Outline

| Print out this category

﻿Overview
Outline
Outline
This chapter describes various codes which are displayed when a failure occurs on the product. These are classified into 3 codes as follows.

Code type | Explanation | Reference
Error code | This code is displayed when an error occurs on the machine. | (Reference)
Jam code | This code is displayed when a jam occurs inside the machine. | (Reference)
Alarm code | This code is displayed when a function of the machine is malfunctioned. | (Reference)

Error code notation
An error code is shown in 7-digit [E000XXX] on the display on the operation panel. However, [000] in 2 to 4 digit is not used. Thus, an error code is described as [EXXX] using 5 to 7 digit in the service manual. (e.g.: E012 = E000012)