Overview

| Print out this category

Test Print﻿
Overview

PG TYPE | Pattern | Image check item | PCB to generate PG
Gradation | Fogging | Transfer failure | Black line | White line | Uneven pitch | Uneven density (rear/ front) | Right angle accuracy Straight line accuracy | Side registration | Shock | Magnification ratio
0 | Normal copy/print |  |  |  |  |  |  |  |  |  |  |  | ---
1 | Grid |  |  |  |  |  |  |  | Yes | Yes |  | Yes | Main Controller PCB 2
2 | 17 gradations Tbic rank 2 | Yes |  |  | Yes | Yes |  |  |  |  |  |  | Main Controller PCB 2
3 | 17 gradations 600dpi (134-line screen or 141-line screen) | Yes |  |  | Yes | Yes |  |  |  |  |  |  | Main Controller PCB 2
4 | Solid white |  | Yes |  |  |  |  |  |  |  |  |  | Main Controller PCB 2
5 | Halftone (density: 80H, Tbic rank 2, without image correction) |  |  | Yes | Yes | Yes | Yes | Yes |  |  | Yes |  | Main Controller PCB 2
6 | Halftone (density: 80H, 134-line screen or 141-line screen, without image correction) |  |  | Yes | Yes | Yes | Yes | Yes |  |  | Yes |  | Main Controller PCB 2
7 | Solid black |  |  | Yes |  | Yes | Yes | Yes |  |  |  |  | Main Controller PCB 2
8 | Horizontal line (4 dots, 27 spaces) |  |  |  | Yes | Yes | Yes | Yes |  |  |  |  | Main Controller PCB 2
9 | Horizontal line (6 dots, 50 spaces) |  |  |  | Yes | Yes | Yes | Yes |  |  |  |  | Main Controller PCB 2
10 | Horizontal line (2 dots, 3 spaces) |  |  |  | Yes | Yes | Yes | Yes |  |  |  |  | Main Controller PCB 2
11 | Halftone (density: 60H, Tbic rank 2, without image correction) |  |  | Yes | Yes | Yes | Yes | Yes |  | Yes | Yes |  | Main Controller PCB 2
12 | Halftone (density: 60H, 134-line screen or 141-line screen, without image correction) |  |  | Yes | Yes | Yes | Yes | Yes |  |  | Yes |  | Main Controller PCB 2
13 | Halftone (density: 30H, Tbic rank 2, without image correction) |  |  | Yes | Yes | Yes | Yes | Yes |  |  | Yes |  | Main Controller PCB 2
14 | Halftone (density: 30H, 134-line screen or 141-line screen, without image correction) |  |  | Yes | Yes | Yes | Yes | Yes |  |  | Yes |  | Main Controller PCB 2
15 | 15 to 50: For development |  |  |  |  |  |  |  |  |  |  |  | ---

NOTE:
When outputting a halftone test print, be sure to use PG TYPE:6 except in the following cases.
1. When checking the image of side registration adjustment, use PG TYPE:11.
2. When the setting value of the following service mode is "2" (TBIC is used for both the photo part and the text part), use PG TYPE:5.
COPIER > OPTION > USER > PH-D-SL2