Setting the Mirroring

| Print out this category

Setting the Mirroring
1) Insert the power plug into the socket and turn on the main power of the host machine.
2) Make a setting of mirroring.
Specify “1” under “Service Mode > COPIER > OPTION > FNCSW > W/RAID”.
3) Turn OFF/ON the main power of the host machine to enable the setting value.
4) Make sure that the UI screen is activated correctly.
5) Make sure that the LED blinks.
HDD1 (Slot 1): The green LED blinks.
HDD2 (Slot 2): The green and red LEDs blink.
CAUTION:
Rebuild process starts after setting “1” for W/RAID. If an error occurs during the rebuild process at the initial installation The hard disk needs to be replaced. (Call service rep.), reexecute the process with the following procedure.
1) Check that the lighting red LED is HDD2.
2) Select Service Mode > COPIER > OPTION > FNCSW > W/RAID, and set “0”.
3) To enable the setting value, turn OFF/ON the Main Power Supply Switch of the host machine.
4) Select Service Mode > COPIER > OPTION > FNCSW > W/RAID, and set "1".
5) To enable the setting value, turn OFF/ON the Main Power Supply Switch of the host machine.
The foregoing procedure is limited to the rebuild process at the initial installation.
An error during the rebuild process that is executed during operation is not included in the consideration.