TPM PCB﻿

| Print out this category

TPM PCB﻿
<Procedure of parts replacement>
. Main Controller PCB 1
<Procedure of adjustment>
When TPM setting is “OFF”
Any operation is not necessary at replacement.
When TPM setting is “ON”
It is necessary to restore the TPM key which was backed up after changing the setting to “ON”.
1) Removing the network cable
Until the TPM key is restored, information might be leaked due to the inappropriate access via network, so be sure to perform this operation appropriately.
2) Connecting the USB Memory after turning ON the main power switch
3) Restoring the TPM key
Management Settings > Data Management >TPM Settings> Restore of TPM Key
4) Turning OFF and ON the main power switch