ANALOG

| Print out this category

ANALOG

COPIER>DISPLAY>ANALOG
TEMP | Display of inside temperature
Lv.1 | Details | To display the temperature inside the machine detected by Environment Sensor.
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 60
Unit | Deg C
Appropriate target value | 20 to 27
Related service mode | COPIER> DISPLAY> ANALOG> HUM, ABS-HUM
HUM | Display of inside humidity
Lv.1 | Details | To display the humidity inside the machine detected by Environment Sensor.
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 100
Unit | %
Appropriate target value | 30 to 70
Related service mode | COPIER> DISPLAY> ANALOG> TEMP, ABS-HUM
ABS-HUM | Display of inside moisture content
Lv.1 | Details | To display the absolute moisture content inside the machine detected by Environment Sensor.
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 100
Unit | g (g/m3)
Appropriate target value | 0 to 22
Related service mode | COPIER> DISPLAY> ANALOG> TEMP, HUM
FIX-C | Display of Fixing Roller center temperature
Lv.1 | Details | To display the center temperature of the Fixing Roller detected by the Fixing Main Thermistor.
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 999
Unit | Deg C
FIX-E | Display of Fixing Roller edge temperature
Lv.1 | Details | To display the edge temperature of the Fixing Roller detected by the Fixing Sub Thermistor 1. Fixing Sub Thermistor 1 is located in the rear nip inlet side of Fixing Roller.
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 999
Unit | Deg C
FIX-UE2 | Display of Fixing Roller edge temperature 2
Lv.1 | Details | To display the edge temperature of the Fixing Roller detected by the Fixing Sub Thermistor 2. Fixing Sub Thermistor 2 is located in the rear nip inlet side of Fixing Roller.
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 999
Unit | Deg C