﻿Enabling UGW Link

| Print out this category

Enabling UGW Link
When installing the firmware in the method of “UGW-linked Download and Update” or “UGW-linked Download”, the following should be set before actually using UGW link.

Service Technician | Setting of Device Service Mode (Level 1) | COPIER >OPTION >FNC-SW >CDS-UGW (0 -> 1)
Setting of UGW WebPortal | In [Customer Management] screen, set [Do not distribute firmware] to [Distribute firmware].
Sales Company's HQ | Setting of Authorities on UGW WebPortal | See "Analysis>Firmware Distribution Information" to grant the appropriate authorities to each account.

NOTE:
See “imageWARE Remote Operator’s Manual / e-Maintenance Business Operation Manual“ for how to operate UGW WebPortal.
[Distribute Firmware] should be set on [Customer Management] screen for staff in charge of setting for [Enter customer information] or [Command for firmware distribution] in order to allow them to select the desired device on [Firmware Distribution Information] screen.