PASCAL

| Print out this category

PASCAL

COPIER>ADJUST>PASCAL
OFST-P-K | Bk density adj at test print reading
Lv.1 | Details | To adjust the offset of Bk color test print reading signal at Auto Adjust Gradation (Full Adjust). When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label. As the greater value is set, the image after adjustment gets darker.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 128
Default value | According to the adjustment value of the Reader at factory shipment