Network Port Settings

| Print out this category

Network Port Settings
The default port of the HTTP server used for MEAP and MEAP applications to provide the servlet function is 8000, and the HTTPS server's default port is 8443. In the case that these ports have already used by the customer who is to introduce this application, the MEAP application cannot use the HTTP (or HTTPS) server(s).
By changing the following ports to use, however, the MEAP application can be used as well as the existing system.
1) Startup level 2 of [ SERVICE MODE ].
2) Press [ COPIER ] > [ Option ] > [ NETWORK ].
3) To specify the HTTP server port, click the [ MEAP-PN ]. To specify the HTTPS (SSL) server port, click the [ MEAP-SSL ].
4) Press the port number to specify on the control panel (the numerical value input in the field is displayed), and press [ OK ] button.
Note:
A port number can be any integer from 0 to 65535. To avoid port numbers that are frequently used, do not use any integer from 0 to 1023.

Server | Setting value | Default value / Value after RAM clear
HTTP Server | 1024 to 65535 | 8000
HTTPS Server | 1024 to 65535 | 8443

Note:
If PS Print Server Unit is connected, do not specify port 8080.
If port 8080 is specified, the RUI of the device where the MEAP authentication application is running cannot be displayed. (Port 8080 is reserved to allow the PS Print Server Unit to redirect to the iR device.)
The HTTPS server port can be used only for devices that support the SSL function.
5) Check to see that it is reflected in setting field, and turn off the main power, and then, restart the device.