Leading Edge Margin Adjustment (1st side)

| Print out this category

Leading Edge Margin Adjustment (1st side)
NOTE:
By executing the leading edge margin adjustment for the Cassette 1, the adjustment is applied to all source of paper.
Execute printing from the Cassette 1, and check that the leading edge margin is within L1=4.0 +1.5mm/-1.0mm.
If it is not within the range, execute adjustment by following the procedure below.
1) Adjust the image position in service mode.
Service mode (Level 1) > COPIER > ADJUST > FEED-ADJ > REGIST
NOTE:
<Setting Range>
-128 to 127 (0.1mm per unit)
As the value is incremented by 1, the leading edge margin is decreased by 0.1mm.
2) Execute duplex printing from the Cassette 1, and check that the left edge margin is within L1=4.0 +1.5mm/-1.0mmmm.
3) When the setting value was changed in step 1), write down the new numerical value in the service label.
4) Exit from the service mode.