Overview

| Print out this category

Version Upgrade via SST
Overview
The system software can be downloaded either of the two modes below via SST.
Assist mode(recommended)
Single mode
Assist mode provides the following features.
Attached option types are automatically recognized.
The new versions of the system software for attached option types are automatically searched.
The set of system software with interactive behavior confirmed is automatically downloaded.
The accessories attached to the host machine are automatically recognized to download the system software for each accessory.
Single mode provides the following features.
The system software download individually are possible.
The HDD format by manual operation are possible.
The service mode password reset are possible.
Upload and the download of data are possible.
This machine holds a number of system software components that mutually interacts during operation. Behaviors of such system software should be confirmed when these are downloaded as the set. Thus, Assist mode is basically recommended to download the system software for this machine.
NOTE:
Use Single mode only when any of the following conditions is met.
When downloading some the system software components, i.e. DCON, RCON or options.
When reloading the system software after HDD is formatted
Downloading the System Software
System software is saved in the temporary storage area on HDD after downloaded with SST.
Restart the machine after download so that it will be written to the system area, and the flash ROM.
After the writing has been completed normally, this machine automatically restarts with the new system software.