DRBL-1

| Print out this category

DRBL-1

COPIER>COUNTER>DRBL-1
TR-ROLL | Transfer Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
Supplement/memo | This is commonly used as operator maintenance parts counter.
SP-SC-EL | Separation Static Eliminator prts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
PT-DRM | Photosensitive Drum parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
DV-UNT-K | Developing Unit parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
C1-PU-RL | Cassette 1 Pickup Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
C1-SP-RL | Cassette 1 Separation Roller parts cntr
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
C1-FD-RL | Cassette 1 Feed Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
C2-PU-RL | Cassette 2 Pickup Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
C2-SP-RL | Cassette 2 Separation Roller prts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
C2-FD-RL | Cassette 2 Feed Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
M-FD-RL | Multifeed Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
M-SP-PD | Multifeed separation Pad prts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
FX-UNIT | Fixing Unit parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
WST-TNR | Waste toner container parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
OZ-FIL1 | Ozone Filter parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0