Send

| Print out this category

Send
* Default Setting
*1 Indicates items that appear only when the appropriate optional equipment is attached.
*4 Indicates item that appears only if the Super G3 2nd Line Fax Board is installed in addition to installing the Super G3 FAX Board.
*5 Indicates item that appears only if the Super G3 3rd/4th Line Fax Board is installed in addition to installing the Super G3 FAX Board.
*6 Indicates item that appears according to the telephone line number specified in [No. of Sending Lines].

Item | Setting Description | Device Information Delivery Available
Output Report
| TX/RX User Data List | Print List | No
| Fax User Data List*1 | Print List | No
Common Settings
| Register Favorite Settings Edit Favorite Settings | Register/Edit, Delete (M1 to M18), Check Content | Yes
|  | Show Comment | On, Off* | Yes
| Display Confirmation for Favorite Settings | On*, Off | No
| Default Screen | Standard*, Address Book, One-Touch, Favorite Settings | No
| Change Default Settings | Register, Initialize | No
| Register Options Shortcuts |  |
|  | Shortcut 1 | 2-Sided Original*, Unassigned | No
|  | Shortcut 2 | Different Size Originals*, Unassigned | No
| TX Report | For Error Only*, On, Off | Yes
|  | Report with TX Image | On*, Off | Yes
| Communication Management Report
|  | Auto Print (100 Transmissions) | On*, Off | Yes
|  | Specify Print Time | On, Off* | Yes
|  | Timer Setting | 00 : 00 to 23 : 59 (00 : 00*) | Yes
|  | Send/Receive Separate | On, Off* | Yes
| TX Terminal ID | Print*, Do Not Print | Yes
| TX Terminal ID: Print Printing Position: Outside Display Destination Unit Name: On, Off Telephone # Mark*1: FAX, TEL | Yes
| Delete Failed TX Jobs | On*, Off | Yes
| Retry Times | 0 to 5 times (3 times*) | Yes
| Data Compression Ratio | High Ratio, Normal*, Low Ratio | Yes
| YCbCr TX Gamma Value | Gamma 1.0, Gamma 1.4, Gamma 1.8*, Gamma 2.2 | Yes
| Use Divided Chunk Send for WebDAV TX | On*, Off | Yes
| Limit New Destinations |  |
|  | Fax | On, Off* | Yes
|  | E-mail | On, Off* | Yes
|  | I-Fax | On, Off* | Yes
|  | File | On, Off* | Yes
| Always Add Device Signature to Send*1 | On*, Off | Yes
|  | Restrict File Formats | On, Off* | Yes
E-mail/Ifax Settings
| Register Unit Name | 24 characters maximum | No
| Communication Settings |  |
|  | SMTP RX | On, Off* | Yes
|  | POP | On* Off | Yes
|  | SMTP Server | Server name or IP Address (48 characters maximum) | No
|  | E-mail Address | 64 characters maximum | No
|  | POP Server | Server name or IP Address (48 characters maximum) | No
|  | POP Address | 64 characters maximum | No
|  | POP Password | 32 characters maximum | No
|  | POP Interval | 0* to 99 (If the interval is set to '0', the incoming e-mail is not checked automatically.) | No
|  |  | POP AUTH Method | Standard*/APOP/POP AUTH | Yes
|  |  | POP Authentication before Sending | On, Off* | No
|  |  | SMTP Authentication (SMTP AUTH) | On, Off* | No
|  |  | User | User name for SMTP authentication (64 characters maximum) | No
|  |  | Password | Password for SMTP authentication (32 characters maximum) | No
|  |  | Allow SSL (POP) | On, Off* | No
|  |  | Allow SSL (SMTP Send) | On, Off* | No
|  |  | Display Auth. Screen When Send | On, Off* | No
|  |  | Allow SSL (SMTP Receive) | Always SSL,On, Off* | No
| Maximum Data Size for Sending | 0=(Off)/1 to 99 MB (3MB*) | Yes
| Default Subject | 40 characters maximum (Attached Image*) | Yes
| Use SMTP Authentication for Each User | On*, Off | No
| Specify Authentication User Dest. to Reply | On, Off* | No
| Set Authorized User Destination to Sender | On*, Off | No
| Allow Sending to Unregistered Destinations | On, Off* | Yes
| Full Mode TX Timeout | 1 to 99 hours (24hours*) | Yes
| Print MDN/DSN upon Receipt | On, Off* | Yes
| Use Send via Server | On, Off* | Yes
| Allow MDN Not via Server | On*, Off | Yes
| Restrict TX Destination Domain |  |
|  | Restrict Sending to Domains | On, Off* | Yes
|  | Permitted Domains | Register, Details/Edit, Delete | No
Fax Settings*1
| Default Screen | Standard*, Address Book | No
| Change Default Settings | Register, Initialize | No
| Register Options Shortcuts
|  | Shortcut 1 | Density*, Unassigned | No
|  | Shortcut 2 | Original Type*, Unassigned | No
|  | Shortcut 3 | 2-Sided Original*, Unassigned | No
|  | Shortcut 4 | Different Size Originals*, Unassigned | No
| Register Sender Name (TTI) | 01 to 99: Register/Edit, Delete | No
| ECM TX | On*, Off | Yes
| Set Pause Time | 1 to 15 seconds (2 seconds*) | Yes
| Auto Redial | On*, Off | Yes
|  | Redial Times | 1 to 10 times (2 times*) | Yes
|  | Redial Interval | 2 to 99 minutes (2 minutes*) | Yes
|  | Redial When TX Error | Error and 1st page*, All pages, Off | Yes
| Check Dial Tone Before Sending | On*, Off | Yes
|  | Fax TX Report | For Error Only*, On, Off | Yes
|  |  | Report with TX Image | On*, Off | Yes
| Fax Activity Report |  |
|  | Auto Print (40 Transmissions) | On*, Off | Yes
|  | Specify Print Time | On, Off* | Yes
|  | Timer Setting | 00: 00 to 23: 59 (00: 00*) | Yes
|  | Send/Receive Separate | On, Off* | Yes
| Set Line
|  | Register Unit Telephone Number | 20 digits maximum | No
|  | Register Unit Name | 24 characters maximum | No
|  | Select Line Type | Pulse, Tone* | No
|  | Line | If the Super G3 FAX Board and Super G3 2nd Line Fax Board are installed: Line 2 | No
|  | If the Super G3 FAX Board, Super G3 2nd Line Fax Board, and Super G3 3rd/4th Line Fax Board are installed: Line 2, Line 3, Line 4 | No
| Select TX Line | If the Super G3 FAX Board is installed: Line 1: Priority TX*, Prohibit TX | No
| If the Super G3 FAX Board and Super G3 2nd Line Fax Board are installed: Line 1: Priority TX*, Prohibit TX Line 2: Priority TX, Prohibit TX | No
| If the Super G3 FAX Board, Super G3 2nd Line Fax Board, and Super G3 3rd/4th Line Fax Board are installed: Line 1: Priority TX*, Prohibit TX Line 2: Priority TX, Prohibit TX Line 3: Priority TX, Prohibit TX Line 4: Priority TX, Prohibit TX | No
| TX Start Speed | 33600 bps*, 14400 bps, 9600 bps, 7200 bps, 4800 bps, 2400 bps | Yes
| PIN Code Access | On, Off* | Yes
| Confirm Entered Fax Number | On, Off* | Yes
| Allow Fax Driver TX | On*, Off | Yes
| Remote Fax TX Settings |  |
|  | Remote Fax Server Address | Host name or the IP address (48 characters maximum) | No
|  | TX Timeout | 1 to 99 hours (24 hours*) | Yes
|  | No. of Sending Lines | 1 to 4 lines (1*) | No
|  | Select Priority Line | Auto*, Line 1, Line 2*6, Line 3*6, Line 4*6 | No
| Remote Fax Settings |  |
|  | Use Remote Fax | On*, Off | Yes