Jam Code List

| Print out this category

Detecting Jams
Jam Code List
Jam in Feed System
xx = 01: Delay, 02: Stationary, 0A: Residue
Yes: Detects, -: Does not detect

Sensor No. | Sensor name | Jam type
Delay | Stationary | Residue
xx01 | S1 | Cassette 1 Pickup Sensor | ○ | ○ | ○
xx02 | S33 | Cassette 2 Pickup Sensor | ○ | ○ | ○
xx05 | S5 | Pre-Registration Sensor | ○ | ○ | ○
xx07 | S19 | Fixing Outlet Sensor | ○ | ○ | ○
xx08 | S21 | No.1 Delivery Sensor | ○ | ○ | ○
xx09 | S22 | No.2 Delivery Sensor | ○ | ○ | ○
xx09 | S24 | Reversal Sensor | - | - | ○
xx0A | S24 | Reversal Sensor | ○ | ○ | ○
xx0D | S7 | Duplex Feed Sensor | ○ | ○ | ○

Other Jams

Sensor No. | Sensor name | Jam type
01FF | S1 | Cassette 1 Pickup Sensor | Sequence error jam
02FF | S33 | Cassette 2 Pickup Sensor | Sequence error jam
05FF | S5 | Pre-Registration Sensor | Sequence error jam
07FF | S19 | Fixing Outlet Sensor | Sequence error jam
08FF | S21 | No.1 Delivery Sensor | Sequence error jam
09FF | S22 | No.2 Delivery Sensor | Sequence error jam
0AFF | S24 | Reversal Sensor | Sequence error jam
0DFF | S7 | Duplex Feed Sensor | Sequence error jam
0B00 | (SW2) | Front Door Switch | Door Open jam(TThe sensor ID is non-display.)
0CA0 | - | time out error jam | command is not received
0CF1 | - | error re-try jam | -