After Installation

| Print out this category

After Installation
1) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
2) Insert the USB Cable and the Control Panel Communication Cable.
3) Install the Right Rear Cover (Upper). (2 Screws)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
4) Connect the power plug of the host machine to the power outlet.
5) Turn ON the main power switch.