﻿Too Large Curl

| Print out this category

Too Large Curl
[Occurrence area]
Fixing assembly
[Cause]
The water content on the front surface of paper becomes different from that on the reverse
side of paper, making the curl larger.
[Occurrence condition]
When the paper has been left alone in a high-humidity environment.
[Remedy]
Service mode (Lv.2)> COPIER> OPTION> IMG-FIX> TMP-TBLC> 0 to 3
0: Auto
1: OFF
2: N1 mode with plain paper 1/2 (Target temperature becomes low.)
3: N3 mode with plain paper 1/2 (Target temperature becomes moreover low.)
Machine shipped with cassette heater: Turn on the heater.
Install an optional cassette heater.