Specification

| Print out this category

Specification

Item | Description
Paper storage method | Front loading method
Pickup method | Cassette | Retard separation method
Manual feed pickup tray | Pad separation method
Paper stack capacity | Cassette | 550 sheets (80 g/m2), 650 sheets (64 g/m2)
Manual feed pickup tray | 80 sheets (80 g/m2), 80 sheets (64 g/m2)
Paper feed reference | Center reference
Paper size | Cassette 1 | A4,A4R,A5R,B4,B5,B5R,LTR,LTTR,LGL,STMTR,EXEC,8K,16K,16KR
Cassette 2 | A4,A4R,A3,A5R,B4,B5,B5R,LTR,LTTR,LGL,11"" x 17"", STMTR,EXEC,8K,16K,16KR, Free size(139.7 mm x 182 mm to 297 mm x 431.8 mm) envelope (No.10(COM10),ISO-B5,ISO-C5,Monarch,DL) *The optional Envelope Feeder Attachment-D1 is required.
Manual feed pickup tray | A4,A4R,A3,A5R,B4,B5,B5R,LTR,LTTR,LGL,11"" x 17"", STMTR,EXEC,8K,16K,16KR, Free size (99 mm x 148 mm to 297 mm x 431.8 mm) envelope (No.10(COM10),ISO-B5,ISO-C5,Monarch,DL) Label (B4,A4R,A4,LTR,LTRR)
Paper grammage | Cassette | 60g/m2 to 128g/m2
Manual feed pickup tray | 52 g/m2 to 220 g/m2
Paper size switch | Cassette | By the user
Manual feed pickup tray | By the user
Duplexing method | Through path