IMG-FIX

| Print out this category

IMG-FIX

COPIER>OPTION>IMG-FIX
FIX-CLN | Set fixing cln sequence execution temp
Lv.2 | Details | To set the execution temperature for the fixing pressure roller cleaning sequence Change the condition (temperature deference between the main thermistor and the sub thermistors) to execute the fixing pressure roller cleaning sequence. When the input value is increased, the execution period is extended.
Use case | When an image failure due to the Pressure Roller occurs
Adj/set/operate method | Enter the setting value, and then press OK key.
Caution | As the short execution interval is set, productivity decreases.
Display/adj/set range | 0 to 3 0: 35 degC 1: 40 degC 2: 45 degC 3: 50 degC
Default value | 0
FIX-TEMP | Setting of down sequence mode
Lv.1 | Details | To set the temperature of the Fixing Assembly to shift to down sequence mode.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

(Productivity priority)
0 to 2: -15 degree
3 to 6: -12 to -3 degree (3 degree unit)
7: OFF
8 to 11: +3 to +12 degree (3 degree unit)
12 to 14: +15 degree
(Fixing grade priority)

Default value | 7
TEMP-CON | Switching of the fixing temp mode: Thick paper
Lv.1 | Details | Switch the fixing temperature mode for thick paper.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

(Productivity priority)
0 to 2: -15 degree
3 to 6: -12 to -3 degree (3 degree unit)
7: OFF
8 to 11: +3 to +12 degree (3 degree unit)
12 to 14: +15 degree
(Fixing grade priority)

Default value | 0
TEMPCON2 | Switching of the fixing temp mode: Manual feed
Lv.1 | Details | Switch the fixing temperature mode when plain paper is fed from the manual feed tray.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

(Productivity priority)
0 to 2: -15 degree
3 to 6: -12 to -3 degree (3 degree unit)
7: OFF
8 to 11: +3 to +12 degree (3 degree unit)
12 to 14: +15 degree
(Fixing grade priority)

Default value | 0
Related service mode | COPIER > OPTION > BODY > FIX-TEMP (Level 1)
FIX-LOW | Fixing performance improvement in low-temp
Lv.1 | Details | This item is used when a fixing failure has occurred in a low-temperature environment.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: Low temperature fixing performance improvement mode is set to ON.
Default value | 0
FX-S-TMP | Set fixing temperature: Curl correction
Lv.1 | Details | To change the fixing temperature to correct the curl, the low fixing and the paper slip in the fixing N mode
Use case | When the curl, the low fixing or the paper slip occurs in the fixing N mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

(Productivity priority)
0 to 2: -15 degree
3 to 6: -12 to -3 degree (3 degree unit)
7: OFF
8 to 11: +3 to +12 degree (3 degree unit)
12 to 14: +15 degree
(Fixing grade priority)

Default value | 7
TMP-TBL2 | Set fixing control temp table: Thin
Lv.1 | Details | To set the control temperature table of the Fixing Roller for 52 to 63g/m2 size paper.
Use case | When alleviating the curl
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -5 to 2 -5 to -1: -5 degC, 0: 0 degC, 1 to 2: +5 degC
Unit | 5 degC
Default value | 0
TMP-TBL4 | Set fixing control temp table: Bond
Lv.1 | Details | To set the control temperature table of the Fixing Roller for bond paper.
Use case | When alleviating the curl
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -5 to 2 -5 to -1: -5 degC, 0 to 2: 0 degC
Unit | 5 degC
Default value | 0
TMP-TBL5 | Set fixing control temp table: Thin
Lv.1 | Details | To set the control temperature table for the thin paper to the S-thin paper mode or the SS-thin paper mode
Use case | For the thin paper which is moist and soft
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: S-thin paper mode (-10 degC compared with Thin paper mode table) 2: SS-thin paper mode (-15 degC compared with Thin paper mode table)
Default value | 0
TMP-TBL6 | Set fixing control temp table: Envelope/Postcard/S-postcard
Lv.1 | Details | To change the fixing control temperature in the envelope mode, postcard mode and S-postcard mode
Use case | When the poor fixing, paper slip or paper curl occurs in the envelope mode, postcard mode and S-postcard mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2: +15 degree 3 to 6: +12 to +3 degree (3 degree unit) 7: OFF 8 to 11: -3 to -12 degree (3 degree unit) 12 to 14: -15 degree
Default value | 7
TMP-TBL7 | Set fixing control temp table: Plain paper 2/Cassette
Lv.1 | Details | To change the fixing control temperature in the plain paper 2 mode at the cassette feeding
Use case | When the poor fixing, paper slip or paper curl occurs in the plain paper 2 mode at the cassette feeding
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2: +15 degree 3 to 6: +12 to +3 degree (3 degree unit) 7: OFF 8 to 11: -3 to -12 degree (3 degree unit) 12 to 14: -15 degree
Default value | 7
RAG-CONT | Set fix smeared image ctrl mode level
Lv.1 | Details | To set level of the mode (skipping) to control smeared image caused by fixing area.
Use case | When a smeared image occurs
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Set RAG-SW to 1 to 3 to enable skipping.
Display/adj/set range | 0 to 3 0: No skipping, 1: Small skipping, 2: Medium skipping, 3: Large skipping
Default value | 0
Related service mode | COPIER> OPTION> IMG-FIX> RAG-SW
FIX-PROT | Measures for jams of paper absorbing moisture
Lv.1 | Details | This item is used when jams occur in paper absorbing moisture.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

0: OFF
1: ON
The mode of measures for jams of paper absorbing moisture (initial rotation period is specified to be longer than the normal period) becomes valid when all the following conditions are satisfied.
- FIX-PROT=""1""
- FIX-TEMP=-10degC or -20degC
- The room temperature is higher than 21degC.

Default value | 0
FIX-OFST | [Not used]
EDG-WAIT | Change of Detection Temp for Fixing Edge
Lv.2 | Details | To change the detection temperature of the fixing sub thermistors 1/2 to switch the paper edge cooling fans to the full speed control, and to shift the machine control to the down sequence
Use case | To reduce the switching frequency of the down sequence, to lower the fixing edge temperature, and to prevent the high temperature offset
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: +20 degC, 1: +10 degC, 2: 0 degC, 3: -10 degC, 4: -20 degC
Default value | 2
TMP-TBLC | Set fixing control temp table: curled paper
Lv.2 | Details | To set the control temperature table to the N1 mode or the N3 mode so that the paper curl is reduced
Use case | When the paper is moist so that the paper curl occurs
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: Auto 1: OFF 2: N1 mode with plain paper 1/2 (Target temperature becomes low.) 3: N3 mode with plain paper 1/2 (Target temperature becomes moreover low.)
Default value | 0 or 1 by models
FIX-PR | Set fixing grade priority mode
Lv.2 | Details | The productivity lowers 4 ppm in the thick paper mode, thick paper H mode and bond paper mode. The productivity lowers 5 ppm in the plain paper mode, thin paper mode and S-thin paper mode when the environment sensor detects less than 18 degC.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON (Fixing grade priority mode)
Default value | 0
TMP-TB12 | Set fixing control temp table: pln/Manual fd
Lv.2 | Details | To change the fixing control temperature in the plain paper 2 mode at the manual feeding
Use case | When the poor fixing, paper slip or paper curl occurs in the plain paper 2 mode at the manual feeding
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2: +15 degC 3 to 6: +12 to +3 degC (3 degC unit) 7: OFF 8 to 11: -3 to -12 degC (3 degC unit) 12 to 14: -15 degC
Unit | 3 degC
Default value | 7
TMP-TB13 | Set fixing control temp table: Thin paper/cst
Lv.2 | Details | To change the fixing control temperature in the thin paper mode at the cassette feeding
Use case | When the poor fixing, paper slip or paper curl occurs in the thin paper mode at the cassette feeding
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2: +15 degC 3 to 6: +12 to +3 degC (3 degC unit) 7: OFF 8 to 11: -3 to -12 degC (3 degC unit) 12 to 14: -15 degC
Unit | 3 degC
Default value | 7
TMP-TB14 | Set fixing control temp table: Thin/Manual fd
Lv.2 | Details | To change the fixing control temperature in the thin paper mode at the manual feeding
Use case | When the poor fixing, paper slip or paper curl occurs in the thin paper mode at the manual feeding
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | "0 to 2: +15 degC 3 to 6: +12 to +3 degC (3 degC unit) 7: OFF 8 to 11: -3 to -12 degC (3 degC unit) 12 to 14: -15 degC"
Unit | 3 degC
Default value | 7
TMP-TB15 | Set fixing control temp table: Pln/2-sided
Lv.2 | Details | To change the fixing control temperature in the plain paper mode 1 during the second printing of 2-sided mode
Use case | When the poor fixing, paper slip or paper curl occurs in the plain paper mode 1 during the second printing of 2-sided mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2: +15 degC 3 to 6: +12 to +3 degC (3 degC unit) 7: OFF 8 to 11: -3 to -12 degC (3 degC unit) 12 to 14: -15 degC
Unit | 3 degC
Default value | 7
TMP-TB16 | Set fixing control temp table: Pln 2/2-sided
Lv.2 | Details | To change the fixing control temperature in the plain paper mode 2 during the second printing of 2-sided mode
Use case | When the poor fixing, paper slip or paper curl occurs in the plain paper mode 2 during the second printing of 2-sided mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2: +15 degC 3 to 6: +12 to +3 degC (3 degC unit) 7: OFF 8 to 11: -3 to -12 degC (3 degC unit) 12 to 14: -15 degC
Unit | 3 degC
Default value | 7