﻿Device's resources

| Print out this category

Device's resources
When 1 MEAP application operates, the resource volume allocated to each device is as follows (loaded resource list). Since the following value is an estimate, when installing the MEAP applications, it needs to check the available resource of SMS.
Since the indication of SMS resource volume fluctuates by the login service (authentication function) and configuration (future model), which the user selected, it may show a bigger value than the following values.
List of Available Resources

Product Name | Storage | Memory | Thread | Socket | File Description
iR-ADV C5051 series | 1024MB | 128MB | 256 | 256 | 256
iR-ADV C9075 series | 1024MB | 128MB | 256 | 256 | 256
iR-ADV 6075 series | 1024MB | 128MB | 256 | 256 | 256
iR-ADV 8105 PRO series | 1024MB | 128MB | 256 | 256 | 256
iR-ADV C2030/ C2025/ C2020 Series | Flash model | 220MB | 32MB | 162 | 128 | 128
HDD model | 1024MB | 128MB | 256 | 256 | 256
iR-ADV 4051 series | 1024MB | 128MB | 256 | 256 | 256

Note:
As for memory, check the available resource when starting up the application. For other resources other than memory, check them when installing.
Some applications call for a specific set of conditions for installation. For details, see the User’s Guide that comes with the individual applications.
Maximum installable application is up to 20 even if the remaining resource is adequate. (However, the Send function consumes 1, it must be 19 in practice.) Authentication application is not included in this number.
The MEAP application, which can be started simultaneously, is up to 19. (Authentication application is not included in this number.)
CAUTION:
To install an application, the user needs to use the following URL when accessing the license control system to obtain a license file. In doing so, he/she needs to register the license access number of the application and the serial number of the device.
http://www.canon.com/lms/license/