FIXING

| Print out this category

FIXING

COPIER>ADJUST>FIXING
FX-FL-SP | Fine adj value entry for fixing film speed when using plain paper
Lv.2 | Use case | When executing RAM clear of DC controller PCB/replacing the PCB
Adj/set/operate method | 1) Select the item to be highlighted to enter the setting value (switch with +/- key), and then press OK key. 2) Turn OFF and then ON the main power switch.
Display/adj/set range | -3 to 3
Unit | msec
Default value | 0
FX-FL-TH | Fine adj value entry for fixing film speed when using thick paper
Lv.2 | Use case | When executing RAM clear of DC controller PCB/replacing the PCB
Adj/set/operate method | 1) Select the item to be highlighted to enter the setting value (switch with +/- key), and then press OK key. 2) Turn OFF and then ON the main power switch.
Display/adj/set range | -3 to 3
Unit | msec
Default value | 0
FX-FL-LW | Fine adj value entry for fix film speed
Lv.2 | Use case | When executing RAM clear of DC controller PCB/replacing the PCB
Adj/set/operate method | 1) Select the item to be highlighted to enter the setting value (switch with +/- key), and then press OK key. 2) Turn OFF and then ON the main power switch.
Display/adj/set range | -3 to 3
Unit | msec
Default value | 0
FN-MV-SW | Change of rotational speed for paper edge cooling fan
Lv.2 | Details | When the rotational speed for the paper edge cooling fan is changed to reduce the curl amount of the moist paper
Adj/set/operate method | 1) Select the item to be highlighted to enter the setting value (switch with +/- key), and then press OK key. 2) Turn OFF and then ON the main power switch.
Display/adj/set range | "0 to 2 0: OFF 1: Half speed 2: Full speed"
Default value | 1
ADJ-FNSH | Open width adj of paper edge cooling fan shutter
Lv.2 | Details | When the open width for the paper edge cooling fan shutter is changed to reduce the curl amount of the moist paper
Adj/set/operate method | 1) Select the item to be highlighted to enter the setting value (switch with +/- key), and then press OK key. 2) Turn OFF and then ON the main power switch.
Display/adj/set range | 0 to 14 0 to 6: Open width is 0 to 24mm (4mm unit) 7 to 14: Open width is 30 to 54mm (4mm unit)
Default value | 7