Installation to the Host Machine

| Print out this category

Installation to the Host Machine
1) Install the HDD Face Plate to the HDD Box.
2 Screws (TP Round End; M3X6)
CAUTION:
Be sure to use the round end screw included in the Removable HDD Kit as the TP screw.
2) Install the HDD Door Unit to the HDD Box.
1 Boss
1 HDD Lock Plate Shaft
1 Hinge Shaft Stopper
3) Remove the plate from the HDD Box. (The removed plate will not be used.)
1 Screw (The removed screw will be used in step 4.)
4) Install the HDD Drawer Unit.
1 Screw (Use the screw removed in step 3.)
5) Install the HDD Box to the HDD Slide Rail.
4 Claws
4 Screws (Use the 4 screws removed in ”Removing the HDD" step 9.)
6) Install the Wire Saddles.
3 Wire Saddles (Large)
3 Wire Saddles (Small)
7) Install the Encryption Board.
4 Screws (TP; M3X4)
CAUTION:
Be sure to put the cables on the Wire Saddle to prevent it from getting under the board.
NOTE:
Be sure to place the side with the 4 connectors in the direction shown in the figure when installing.
Tighten the screws in the order shown in the figure.
8) Install the LED Board (A:LED) .
1 Boss
1 Screw (TP; M3X4)
9) Connect the LED Cable (A:LED-Sig) .
2 Connectors
1 Plastic Film Sheet
3 Wire Saddles (Small)
10) Connect the cables of the HDD Drawer Unit.
2 Connectors of the Signal Cable
2 Connectors of the Power Supply Cable
NOTE:
Be sure to connect "A:HDD-Sig1" (red) and "A:HDD-Pow1" to CH-A of the PCB.
Be sure to connect "A:HDD-Sig2" (blue) and "A:HDD-Pow2" to CH-B of the PCB.
11) Secure the cables in place using the Wire Saddles.
3 Wire Saddles (Large)
NOTE:
Be sure to secure the LED Cable (A:LED-Sig) in place together with other cables using the Wire Saddle [A].
12) Disconnect the 2 cables. (The 2 removed cables will not be used.)
2 Connectors
2 Wire Saddles
3 Edge Saddles
13) Install the Signal cable (A:Cont-Sig) and Power cable (A:Cont-Pow).
3 Edge Saddles
2 Wire Saddles
2 Connectors
14) Return the HDD Unit to the host machine.
NOTE:
Be sure to move the unit in the direction of the arrow when installing it to prevent the protrusion of the HDD Slide Rail from coming in contact with the plate of the host machine.
Be sure not to push the Signal cable (A:Cont-Sig) and the Power cable (A:Cont-Pow) into the host machine.
15) Connect the Connector of the Signal cable (A:Cont-Sig) and the Connector of the Power cable (A:Cont-Pow).
1 Wire Saddle
NOTE
When connecting the connector, be sure to connect it with the terminals inside the connector is on the rear side.
Be sure to pass the Signal cable (A:Cont-Sig) and the Power cable (A:Cont-Pow) through the Wire Saddle when connecting.
16) Secure the HDD Unit.
2 Screws (Use the screws removed in "Removing the HDD" step 8.)
CAUTION:
Be careful not to drop the screw.
Be sure to tighten the screws in the order shown in the figure.
17) Close the plate.
18) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
19) Connect the USB Cable and the Control Panel Communication Cable.
20) Install the covers.
Controller Box Cover
Rear Cover (4 Screws) (Tighten the screws in the following order: upper left, lower left, upper right, and then lower right.)
Right Rear Cover (2 Screws)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
21) Open the Small Cover of the Right Rear Cover, and affix the label.
1 Shutdown Cuution Label
1 LED Label
22) Open the HDD Door Unit.
23) Install the Removable HDD 1 (front).
NOTE:
Be sure to insert it until it stops.
24) Close the HDD Door Unit.
25) Be sure to request the user to padlock the removable HDD to discourage theft.
26) Close the Small Cover of the Right Rear Cover.