Preparation before Installation

| Print out this category

Installation Procedure
Preparation before Installation
1) Remove the Right Rear Cover (Upper).
2 Screws
2 Protrusions
1 Claw
2) Disconnect the USB Cable and the Control Panel Communication Cable.
3) Remove the Main Controller PCB 1.
2 Screws (beside of arrow mark)
1 Connector
CAUTION:
Be sure to move the USB Cable and the Control Panel Communication Cable to the Reader side to prevent the cables from being trapped.
CAUTION:
Be sure to place the removed Main Controller PCB 1 on flat surface.
Reason: Since the fan protrudes, if it is placed at a tilt, it may be damaged.