ADJUST

| Print out this category

ADJUST

FEEDER>ADJUST
DOCST | Adj of DADF img lead edge margin: front
Lv.1 | Details | To adjust the margin at the leading edge of the image for DADF scanning. Execute when the output image after DADF installation is dislocated. When replacing the Reader Controller PCB/clearing RAM data, enter the value of service label. As the value is incremented by 1, the margin at the leading edge of the image is decreased by 0.1mm. (The image moves in the direction of the leading edge of the sheet.)
Use case | - When installing DADF - When replacing the Reader Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.1 mm
LA-SPEED | Fine adj of DADF image magnifictn: front
Lv.1 | Details | To adjust the image magnification in vertical scanning direction for DADF scanning. As the value is incremented by 1, the image is reduced by 0.1% in vertical scanning direction. (The feeding speed increases, and the image is reduced.)
Use case | - When installing DADF - When replacing the Reader Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -30 to 30
Unit | 0.10%
DOC-LNGH | DADF paper detection adj for the long sheet/free size mode
Lv.1 | Details | When DADF is installed (to adjust the detection margin of error for the long sheet/free size mode)
Use case | - When installing DADF - When replacing the Reader Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -100 to 100
Unit | 0.1mm