AE

| Print out this category

ADJUST
AE

COPIER>ADJUST>AE
AE-TBL | Adj of text density at image density adj
Lv.1 | Details | To adjust text density according to the adjusted image density. When clearing the RAM data of the CCD unit (CCD PCB), enter the value of service label. As the greater value is set, text gets darker.
Use case | When clearing the RAM data of the CCD unit (CCD PCB)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 9
Default value | 5