Network configuration process

| Print out this category

Device Settings
Network configuration process
To support a MEAP-enabled iR device via network (SMS, etc.), set up the network setting on the touch panel of the iR device (this setting is [ ON ] by default).
1) Press [ Settings/Registration ] button, select [ Preferences ] > [ Network ] > [ TCP/IP Settings ] > [ Use HTTP ] and press [ On ] button.
Note:
In iR-ADV series, the System Manager ID and the System PIN are configured by default, so “Network” and the items that follow are grayed out and cannot be selected.
Return to the top screen, press “Login” button at the lower left of the screen, login as the system manager, and configure the settings.
The default setting for the System Manager ID is “7654321”, and the password is” 7654321”.
Note:
When using SSL, press [Settings/ Registration] button, select [Management Settings]>[License / Other] > [MEAP Settings] > [SSL Settings] and press [On] button. (This setting is applied to SSL setting on RUI. Vice versa, [On] set for SSL on RUI is also applied to the touch panel.)
When [Use SSL] is set to On, the message dialog, [The Default Key is not set. Check the Key and Certificate List settings in Certificate Setting.], is shown. Press [OK] button for this message.
2) Press [ OK ] button to return to Main Menu screen.
3) Restart the device.
CAUTION:
The setting [ Use HTTP ] is not actually enabled/disabled until you have restarted the device.
You cannot make a connection through a proxy server. If a proxy server is in use, enter the IP address of the MEAP device in the Exceptions field for the browser. Open Internet Options dialog of Internet Explorer and select Connections tab, LAN Settings button, Use a proxy server option, and Advanced button of Proxy server group. Proxy Settings dialog will opens. The Exceptions field is in the dialog. As network settings vary among environments, consult the network administrator.
If Cookie and JavaScript are not enabled in the Web browser, you will not be able to use SMS.
To type text using the Web browser, use the characters compatible with the MEAP device’s touch panel display. The MEAP device may not properly recognize some characters.
When [Use SSL] is made available, it is necessary to set the key and the certificate necessary for the SSL communication. Set the key and the certificate by SSL with [SSL Settings] that exists in [Preferences] > [Network] > [TCP/IP Settings] > [SSL Settings] on the iR device.