IMG-LSR

| Print out this category

IMG-LSR

COPIER>OPTION>IIMG-LSR
COTDPC-D | Toner usage reduction mode: Decrease VD
Lv.2 | Details | Reduce toner usage. (The potential VD is decreased.)
Adj/set/operate method | 1) Switch with +/- key, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: No reduction 1: Reduction by approx. -10% 2: Reduction by approx. -20% 3: Reduction by approx. -30%
Default value | 0
SC-PR-SW |  | Set scanner last rotation time
Lv.2 | Details | To stop the polygon motor immediately after the last rotation so that a noise of the polygon motor is reduced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0