Checking after Installation

| Print out this category

Checking after Installation
1) Enter Service Mode, and set the model of the Card Reader.
Check the service mode (COPIER > OPTION > ACC > CR-TYPE) to see that the setting value is "0".
NOTE:
Upon user's request, number of cards (departments) can be changed. This setting change must be performed before performing step 2.
Select Service Mode (Level 2) > COPIER > OPTION > FNC-SW > CARD-RNG, and set any value.
Turn OFF and then ON the main power switch to enable the setting value.
After that, perform from step 1.
2) Enter Service Mode > COPIER > FUNCTION > INSTALL > CARD, and enter the card number to be used (1 to 2001).
Enter the smallest card number to be used by a user.
From the entered card number, 1000 cards can be used.
3) Turn OFF and then ON the main power switch to enable the setting value.
4) Insert a card which card number has been registered, and check that the machine moves to standby condition.
NOTE:
When changing number of cards (departments) upon user's request after specifying the setting, specify the following settings. In such a case, the department ID counter information is reset.
Select Service Mode > COPIER > FUNCTION > CLEAR > CARD.
Select Service Mode (Level 2) > COPIER > OPTION > FNC-SW > CARD-RNG, and set any value.
Select Service Mode > COPIER > FUNCTION > INSTALL > CARD, and enter the card number to be used (1 to 2001).
Turn OFF and then ON the main power switch to enable the setting value.
After that, perform from step 1.