Service cautions

| Print out this category

Service cautions
1) After performing the following service actions, it is necessary to perform initializing E-RDS settings (ERDS-DAT) and communication test (COM-TEST).
Failure to do so will result that the counter transmitting value to the UGW may become unusual.
RAM clear of MNCON PCB SRAM Board :
[SERVICE MODE] > [COPIER] > [Function] > [CLEAR] > [MN-CON]
Also, after replacing the main controller board, all settings must be reprogrammed.
2) The following settings in service mode must not be change unless there are specific instructions to do so. Changing these values will cause error in communication with UGW.
Set port number of UGW
[SERVICE MODE] > [COPIER] > [Function] > [INSTALL] > [RGW-PORT]
Default : 443
URL setting of UGW
[SERVICE MODE] > [COPIER] > [Function] > [INSTALL] > [RGW-ADR]
Default : https://a01.ugwdevice.net/ugw/agentif010