Shading Correction (Overview)

| Print out this category

Shading Correction (Overview)
The output of the CCD is not necessarily even for the following factors even when the density of the original is uniform:
1) Variation in the sensitivity of the CCD among pixels
2) Variation in the intensity of the rod lens array
3) Variation in the intensity of light that goes through the center and surroundings of lens
4) Variation in the intensity of light at the center and surroundings of LED
5) LED deterioration
The machine executes shading correction to even out the output of the CCD.
Shading correction may be the shading correction executed for each job.