﻿Removing the Manual Feed Separation Pad

| Print out this category

﻿Removing the Manual Feed Separation Pad
CAUTION:
Do not touch the pad surface during work.
1) Remove the manual feed pickup roller. (Reference)
2) Slide the bushing (rear) backward.
1 claw
3) Remove the separation pad with a flat-blade screwdriver.
NOTE:
Insert a screwdriver diagonally.
NOTE:
When replacing the consumable parts, be sure to clear the parts counter.
(COPIER > COUNTER > DRBL-1 > M-SP-PD)