CCD

| Print out this category

CCD

COPIER>DISPLAY>CCD
TARGET-B | Shading target value (B)
Lv.2 | Details | To display the shading target value of Blue. Continuous display of 0 (minimum) or FFFF (maximum) is considered a failure of the CCD unit (CCD PCB).
Use case | - When replacing the CCD unit (CCD PCB) - At scanned image failure
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to FFFF
Appropriate target value | 512 to 2047
TARGET-G | Shading target value (G)
Lv.2 | Details | To display the shading target value of Green. Continuous display of 0 (minimum) or FFFF (maximum) is considered a failure of the CCD unit (CCD PCB).
Use case | - When replacing the CCD unit (CCD PCB) - At scanned image failure
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to FFFF
Appropriate target value | 512 to 2047
TARGET-R | Shading target value (R)
Lv.2 | Details | To display the shading target value of Red. Continuous display of 0 (minimum) or FFFF (maximum) is considered a failure of the CCD unit (CCD PCB).
Use case | - When replacing the CCD unit (CCD PCB) - At scanned image failure
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to FFFF
Appropriate target value | 512 to 2047
OFST-B | CCD offset level adj value (blue)
Lv.2 | Details | To display the CCD offset level value for blue
Use case | When image failure is caused by CCD, check whether the adjustment value is proper or not.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
OFST-G | CCD offset level adj value (green)
Lv.2 | Details | To display the CCD offset level value for green
Use case | When image failure is caused by CCD, check whether the adjustment value is proper or not.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
OFST-R | CCD offset level adj value (red)
Lv.2 | Details | To display the CCD offset level value for red
Use case | When image failure is caused by CCD, check whether the adjustment value is proper or not.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
OFST-O | Adj value of offset level in odd bit on CCD
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
OFST-E | Adj value of offset level in even bit on CCD
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
GAIN-B | Adj value of gain level on CCD (blue)
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
GAIN-G | Ad value of gain level on CCD (green)
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
GAIN-R | Adj value of gain level on CCD (red)
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
GAIN-O | Adj value of gain level in odd bit on CCD
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
GAIN-E | Adj value of gain level in even bit on CCD
Lv.2 | Details | To judge if this adjustment value is correct when an image fault attributed to CCD occurs.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
MFIL | MTF adj index for main scanning direction
Lv.2 | Details | Display of MTF adjustment for the main scanning direction
Use case | When the image fault is caused by CCD, ensure whether the adjustment value is proper or not.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255
SFIL | MTF adj index for sub scanning direction
Lv.2 | Details | Display of MTF adjustment for the sun scanning direction
Use case | When the image fault is caused by CCD, ensure whether the adjustment value is proper or not.
Adj/set/operate method | N/A (Display only)
Appropriate target value | 0 to 255