Installation Procedure

| Print out this category

Installation Procedure
1) Loosen the 2 screws, and move the Utility Tray Mounting Plate in the direction of the arrow until it stops.
2) While pulling the [A] part of the Utility Tray, remove the Utility Tray Mounting Plate.
Utility Tray (The removed Utility Tray will be used in step 5.)
Utility Tray Mounting Plate (The removed Utility Tray Mounting Plate will be used in step 4.)
CAUTION:
Be sure not to pull the [A] part of the Utility Tray too much.
3) Remove the 5 Face Seals from the Reader Right Cover.
(The removed Face Seals will not be used.)
4) Install the Utility Tray Mounting Plate.
(Use the Utility Tray Mounting Plate removed in step 2.)
5 Screws (TP; M4x8)
5) Install the Utility Tray. (Use the Utility Tray removed in step 2.)
2 Screws (TP; M4x8)
2 Screws (Tighten the screws loosened in step 1.)