Compatibility among Device, Encryption PCB and HDD

| Print out this category

Compatibility among Device, Encryption PCB and HDD
E602-2000 error may occur if the unmatched authentication information is found between the controller and the HDD Encryption PCB and the Encryption PCB is mounted.
The device, the Encryption PCB and HDD can be connected in 4 use cases.
Case 1: Normally operated
Case 2: HDD-related error (other than E602-2000) occurs because the system on the HDD cannot be read
Case 3: E602-2000 error is triggered by failure in mutual authentication
Case 4: Unable to decode properly due to unmatched key for the Encryption PCB