ENV-SET

| Print out this category

ENV-SET

COPIER>OPTION>ENV-SET
ENVP-INT | Temp, humid/Fix Roll temp log get cycle
Lv.1 | Details | To set the cycle to obtain log of the temperature and humidity inside the machine or the surface temperature of the Fixing Roller. As the value is incremented by 1, the cycle is increased by 1 minute. Obtained log can be displayed by selecting the following: COPIER > DISPLAY > ENVRNT
Use case | At trouble analysis
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 480
Unit | 1 minute
Default value | 60
Related service mode | COPIER> DISPLAY> ENVRNT
IMG-BLD1 | Set condensation prevention mode
Lv.2 | Details | To warm the developing unit, drum unit and the parts around them, the fixing initial rotation is carried out. When the value is increased, the effect becomes big.
Use case | When image smear occurs
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: Level 1 (Charge current is decreased.) 2: Level 2 (In addition to level 1, the ON time of the transfer roller cleaning is extended 30 sec.) 3: Level 3 (In addition to level 2, the initial rotation is extended 240 sec.)
Default value | 0
IMG-BLD2 | Set image smear prevention mode
Lv.2 | Details | When the high temperature and high humidity is detected, the frequency of the primary charge is changed from 1838Hz to 1050Hz.
Use case | When the image smear occurs in the high temperature and high humidity environment
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0
IMG-BLD3 | Set image smear prevention mode 3
Lv.2 | Details | To prevent the image smear in the high humidity, the cleaning ability of the drum surface is raised by this mode and the deteriorated toner is removed. When the value is increased, the effect becomes big.
Use case | When the image smear occurs.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The toner consumption is increased and it influences the dirt of the transfer roller.
Display/adj/set range | 0: OFF 1: Mode 1 2: Mode 2 3: Mode 3
Default value | 0