﻿Thin Paper Jam (63g/m2 or Less)

| Print out this category

Thin Paper Jam (63g/m2 or Less)
[Occurrence area]
Drum
Fixing assembly
[Cause]
The separation power reduces due to low elasticity of paper, causing a jam in the drum assembly or fixing assembly.
[Occurrence condition]
When paper thinner than 64g/cm2 paper is used.
[Remedy]
Service mode (Lv.1)> COPIER> OPTION> IMG-FIX> TMP-TBL5> 0 to 2
0: OFF
1: S-thin paper mode (-10 degC compared with Thin paper mode table)
2: SS-thin paper mode (-15 degC compared with Thin paper mode table)