Specification of SSO-H

| Print out this category

Specification of SSO-H

Item | Specification
No. of local device users | Up to 5000
Maximum number of domains | 200 domains (“this device” not included)
Supported device | All the MEAP-enabled iR devices (different SSO-H versions are supported depending on machine types)
IPv6 | Authentication provided in IPv6 supports AD/KDC/DNS of Windows Server 2008 only)
Memory (KB) / thread (numbers) | 3584/33
Supported Active Directory | Windows 2000 Server SP4/ Windows Server 2003 SP1/Windows Server 2003 R2/ Windows 2008 Server(64BitOS not supported)
Availability of Department Management Linkage | Available only in local authentication
Site access | Supported

SSO/SDL handling
Conventional SSO and SDL are not packaged in Administrator's CD of this model. In addition, this model does not support older versions of SSO or SDL released in the past.