Security Information Storage Location

| Print out this category

Security Information Storage Location

Storage Location | Data Type | Function | Name of Data | Backup Availability
HDD | Password/ PIN | BOX | BOX Password | Yes
HDD | Password/ PIN | BOX | Password for Fax BOX | Yes
HDD | Password/ PIN | SEND | Password for a file destination of Address Book | Yes
HDD | Password/ PIN | MEAP | Authentication information registered by local device authentication via SSO-H | Yes
HDD | Certificate/ Secret Key | SSL,AMS | Device key pair (SSL, AMS) | No
HDD | Certificate/ Secret Key | Signature SEND | User key pair | No
HDD | Others | User setting information | Key information linked to user (password) | No
SRAM | Password/ PIN | BOX | Password for encryption at BOX backup | No
SRAM | Password/ PIN | BOX | Password for SMS server at BOX backup | No
SRAM | Password/ PIN | Advanced BOX | Password for Advanced BOX backup | No
SRAM | Password/ PIN | Advanced BOX | Password for SMS server at Advanced BOX backup | No
SRAM | Password/ PIN | SEND | Password for LDAP server | Yes
SRAM | Password/ PIN | SEND | Password for POP3 server | Yes
SRAM | Password/ PIN | SEND | Password for time-stamped PDF | Yes
SRAM | Password/ PIN | SEND | Password for Adobe ES Rights Management Server | Yes
SRAM | Password/ PIN | SEND | PIN for destination list (in destination setting) | Yes
SRAM | Password/ PIN | UI | Password for service mode | No
SRAM | Password/ PIN | Network | Password for IPP authentication | Yes
SRAM | Password/ PIN | Network | Password for FTP authentication | Yes
SRAM | Password/ PIN | Network | User name and password for client in Proxy authentication | Yes
SRAM | Password/ PIN | Network | Login password for Netware print server | Yes
SRAM | Password/ PIN | Network | Policy common key for IPSec | Yes
SRAM | Password/ PIN | Network | User name and password for PEAP/TTLS authentication | Yes
SRAM | Password/ PIN | Others | Password for FAX receipt | Yes
SRAM | Password/ PIN | Others | Department management data (including System Manager password) | Yes
SRAM | Encryption key | MIB | Authentication and encryption keys for SNMPv3 | No