Change of the fixing grade with the other service modes

| Print out this category

Change of the fixing grade with the other service modes
The following service modes influence the fixing grade in addition to the service modes described above.

Service mode | Outline | Setting value | Fixing temperature control / Throughput
Curl correction mode for plain paper COPIER >OPTION >IMG-FX >TMP-TBLC | The fixing temperature is changed in the plain paper 1 mode and plain paper 2 mode. The fixing grade is improved by lowering the productivity. | 0 (Auto) (Fixing grade improvement) | Change the normal temperature control and N1 mode (*1) according to the environment (temperature/humidity)
1 (Off) (Default) | Normal temperature control (plain paper mode control)
2 (Medium) (Fixing grade improvement) | N1 mode temperature control
3 (High) (Fixing grade improvement) | N3 mode (*2) temperature control
Curl correction mode for thin paper COPIER >OPTION > IMG-FX >TMP-TBL5 | The fixing temperature is changed in the thin paper mode. The fixing grade is improved by lowering the productivity. | 0 (Off) (Default) | Normal temperature control (plain paper mode control)
1 (Medium) (Fixing grade improvement) | S-thin paper mode temperature control (The control temperature of thin paper mode is lowered by 10 deg C uniformly.)
2 (High) (Fixing grade improvement) | SS-thin paper mode temperature control (The control temperature of thin paper mode is lowered by 15 deg C uniformly.)
Fixing grade improvement mode COPIER >OPTION >IMG-FX >FIX-PR | The fixing temperature is changed in the thick paper 1/2/3/4 mode and bond paper mode, and also the plain paper 1/2 mode and thin paper mode under the prescribed environment. | 1 (Off) (Default) | Normal control
2 (On) (Fixing grade improvement) | The throughput of every size paper is lowered by 4 cpm in the thick paper 1/2/3/4 mode and bond paper mode. The throughput of every size paper is lowered by 5 cpm in the plain paper 1/2 mode and thin paper mode when the environment sensor detects less than 18 dreg C.
Loosened down sequence mode COPIER >OPTION >BODY >PSP-PR1 | The print speed-down is loosened at the temperature rise of non-feeding area. The productivity has priority over the fixing grade by shortening the wait time at the size change. (*3) | Off (Default) | The temperature difference between the main thermistor and the sub thermistor for allowing the pick up operation is 20 degree C.
On (Productivity improvement) | The temperature difference between the main thermistor and the sub thermistor for allowing the pick up operation is 30 degree C.
Productivity priority mode in rotation collation COPIER >OPTION >ENV-SET >PSP-PR4 | The productivity has priority over the fixing grade by shortening the wait time at the rotation collation mode. | 0:OFF (Default) | Normal control
Image Priority | The temperature difference between the main thermistor and the sub thermistor for allowing the pick up operation is 20 degree C.
Speed Priority 1 (Productivity improvement) | The temperature difference between the main thermistor and the sub thermistor for allowing the pick up operation is 40 degree C.
Speed Priority 2 (Productivity improvement-high) | The temperature difference between the main thermistor and the sub thermistor for allowing the pick up operation is 60 degree C.

*1. N1 mode: "Normal control temp." - 15 degree C (when the fixing temperature is 100 degree C or more at the start of warm up control)
*2. N3 mode: "Normal control temp." - 48 degree C (when the fixing temperature is 100 degree C or more at the start of warm up control)
*3. The set value of the productivity priority mode has priority at the rotation collation mode.