Jam Type

| Print out this category

Jam Code
Jam Type
Jam types are shown below.

Type | Meaning
DELAY | Delay jam
STNRY | Stationary jam
OVERLAP | Double feed detection
TIMING NG | Timing error
OHP NG | Incorrect paper
ADF OP | ADF open
COVER OP | Cover open
RESIDUAL | Residual jam
PICKUP NG | Pickup error
POWER ON | Power ON
DOOR OP | Door open
SEQ NG | Sequence jam
DELAY ESC | Delay jam while ejecting to the escape delivery tray
OTH JAM | Other jams
STNRY ESC | Stationary jam while ejecting to the escape delivery tray
STP | Staple
SDL STP | Saddle stitch staple
INIT ROT | Residual (at initial rotation)
UP DEVICE | Upper stream device jam
OTHER | Others
ERROR | Error
RETRY ERR | Retry error
STOP | Press Stop key
ROT | Keeps rotating
PROGRAM | Program
TIME OUT | Time-out
PUNCH | Punch
MEDIA NG | Misprint