Setting values and data to be initialized

| Print out this category

Setting values and data to be initialized
The following E-RDS settings, internal data, and Alarm filtering information are initialized.
COPIER > Function > INSTALL > E-RDS
COPIER > Function > INSTALL > RGW-ADR
COPIER > Function > INSTALL > RGW-PORT
COPIER > Function > INSTALL > COM-LOG
CAUTION:
In case of replacing the CA certificate file, even if initialization of E-RDS is executed, the status is not returned to the factory default.
When installing the certificate file other than the factory default CA certificate file, it is required to delete the certificate file after E-RDS initialization and install the factory default CA certificate file.
For detailed procedures, see "Steps to E-RDS settings - step 3.".