Paper Deck Unit-B2

| Print out this category

Paper Deck Unit-B2

ACC ID | Jam Code | Type | Sensor ID | Sensor Name/Description
00 | 010F | DELAY | PS6D | Deck pickup sensor
00 | 020F | STNRY | PS6D | Deck pickup sensor
00 | 0A0F | POWER ON | PS6D | Deck pickup sensor
00 | FF0F | SEQ NG*1 | PS6D | Deck pickup sensor

*1: The state is recovered by opening and closing the Door, or turning OFF and then ON the power supply.
If it is not recovered by the above operation, it is considered an error near the target sensor.
Disconnect and then connect the connectors around the target sensor, check if the cable is open circuit, and replace the sensor.