Domain authentication

| Print out this category

Domain authentication
This is a form of user authentication which operates in collaboration with the domain controller on the Active Directory environment network and, as soon as the iR device is logged into, carries out authentication of the domain on the network. In addition to users belonging to the domain that includes the iR device, users belonging to domains that have a reliable relationship with the domain (multi-domain) can also be authenticated. The domain name of the login destination can be selected by the users themselves upon login.
The function makes use of options iW EMC Accounting Management Plig-in to enable analysis and management of the iR device usage status.
The protocol used is as follows.
Kerberos:LLS/RLS/ILS
NTLMV2:WLS(Web Service Login Service)
User information acquisition is done by LDAP, so the Active Directory LDAP port needs to be made accessible. If LDAP connection fails, the authentication will end in error.
No. of supported domains: 200 (unchanged from SSO) Site access supported.
Differences from conventional SSO