﻿Removing the HDD

| Print out this category

﻿Removing the HDD
Removing the Covers
1) Remove the Right Rear Cover (Upper).
2 Screws
2 Protrusions
1 Claw
2) Remove the Rear Cover.
4 Screws
4 Claws
3) Remove the Controller Box Cover.
6 Hooks
Removing the Cables
4) Disconnect the USB Cable and the Control Panel Communication Cable.
Removing the Main Controller PCB 1
5) Remove the Main Controller PCB 1.
2 Screws (beside of arrow mark)
1 Connector
CAUTION:
Be sure to move the USB Cable and the Control Panel Communication Cable to the Reader side to prevent the cables from being trapped.
Removing the HDD Unit
6) Open the plate in the direction of the arrow.
2 Hooks
7) Disconnect the 2 cables.
2 Connectors
1 Wire Saddle
8) Remove the HDD Unit.
2 Screws
CAUTION:
Be careful not to drop the screw.
Pull out the HDD Unit until it stops, and then move it in the direction of the arrow to remove.
Be careful not to drop the HDD Unit.
9) Remove the HDD Box from the HDD Unit.
4 Screws
10) Remove the HDD Fixation Plate Unit from the HDD Box.
2 Screws
NOTE:
When removing the HDD Fixation Plate Unit, it clicks.
﻿