﻿Removing the Cassette Separation Roller

| Print out this category

Removing the Cassette Separation Roller
CAUTION:
Do not touch the roller surface during work.
1) Draw out the cassette from the main unit.
2) Open the right cover.
3) Remove the cassette separation roller.
1 claw
NOTE:
When replacing the consumable parts, be sure to clear the parts counter.
- Cassette 1 (COPIER > COUNTER > DRBL-1 > C1-SP-RL)
- Cassette 2 (COPIER > COUNTER > DRBL-1 > C2-SP-RL)