INT-FACE

| Print out this category

INT-FACE

COPIER>OPTION>INT-FACE
IMG-CONT | [Not used]
NWCT-TM | Timeout setting of network connection
Lv.2 | Details | To set the time to keep network connection between this machine and the PC application (keep-alive setting). As the value is incremented by 1, the time is increased by 1 minute.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 5
Unit | 1 minute
Default value | 5
Supplement/memo | Expected PC application: Network print application, E-mail function, cascade copy, MEAP network application, etc.
CNT-TYPE | [Not used]