Firmware to be exported to USB memory

| Print out this category

Firmware to be exported to USB memory
When the firmware of the selected optional language in "Optional Language Setting" is installed to SST, it is exported to the USB memory.
The firmware of the other optional languages are not exported to the USB memory.
When Danish and Dutch are selected in the "Optional Language Setting", the firmware of these languages are exported to the USB memory as shown below.