FNC-SW

| Print out this category

OPTION
FNC-SW

COPIER>OPTION>FNC-SW
MODEL-SZ | Fixed magnifictn & DADF orgnl dtct size
Lv.1 | Details | To set the fixed magnification ratio display and the original detection size with DADF. It is set automatically at the time of installation of the Reader according to the location.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 3 0: AB configuration (6R5E) for Japan, 1: Inch configuration (5R4E) for North/Middle/South America, 2: A configuration (3R3E) for Europe, 3: AB/Inch configuration (6R5E) for Asia, Oceania, South America
Default value | It differs according to the location.
SCANSLCT | ON/OFF of scan area calculate function
Lv.2 | Details | To set ON/OFF of the function to calculate scanning area from the specified paper size. When the paper size is larger than the original size, selecting ON reduces productivity because the scanning area gets larger.
Use case | When matching the scanning area with the paper size
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF (calculated from the detected original size) 1: ON (calculated from the specified paper size)
Default value | 0
SENS-CNF | Setting of original detection size
Lv.2 | Details | To set original detection size according to AB configuration/Inch configuration/A configuration. Select 1 (Inch configuration) for Inch configuration/A configuration machine.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: AB configuration, 1: Inch configuration
Default value | 0
CONFIG | Set country/area/lang/location/ppr size
Lv.1 | Details | To set the country/region, language, location, paper size configuration for multiple system software in HDD.
Use case | Upon user's request
Adj/set/operate method | 1) Select the setting item. 2) Switch with +/- key, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

XX YY.ZZ.AA
XX: Country/region
JP: Japan, US: United States, GB: England, FR: France, DE: Germany, IT: Italia, AU: Australia, SG: Singapore, NL: Netherlands, KR: Korea, CN: China, TW: Taiwan, ES: Spain, SE: Sweden, PT: Portugal, NO: Norway, DK: Denmark, FI: Finland, PL: Poland, HU: Hungary, CZ: Czech, SI: Slovenia, GR: Greek, EE: Estonia, RU: Russia, AD: Andorra, AL: Albania, AM: Armenia, AR: Argentine, AT: Austria, BA: Bosnia Herzegovina, BE: Belgium, BG: Bulgaria, BO: Bolivia, BR: Brazil, CA: Canada, CH: Switzerland, CL: Chile, CY: Cyprus, HR: Croatia, ID: Indonesia, IE: Ireland, IL: Israel, IN: India, IS: Iseland, LU: Luxembourg, LV: Latvia, MX: Mexico, MY: Malaysia, NZ: New Zealand, PE: Peru, PH: Philippine, PY: Paraguay, RO: Romania, SK: Slovakia, TH: Thailand, TR: Turkey, UA: Ukraine, UY: Uruguay, VE: Venezuela, VN: Vietnam
YY: Language (Fixed; e.g. ja: Japanese)
ZZ: Location (Fixed; e.g. 00: CANON)
AA: Paper size configuration (00: AB configuration, 01: Inch configuration, 02: A configuration, 03: Inch/AB configuration)

Related service mode | COPIER> OPTION> FNC-SW> MODEL-SZ
W/SCNR | Setting of Reader Unit installation
Lv.1 | Details | To set installation of the Reader Unit. 1 (Installed) is automatically selected once the Reader Unit is detected at the start of the machine.
Use case | When installing/removing the Reader Unit
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Not installed, 1: Installed
Default value | According to the setting at shipment
FAN-EXTN | Fan drive extension mode after job
Lv.2 | Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0
ORG-LGL | Special paper size set in DADF mode: LGL
Lv.2 | Details | To set the size of special paper (LGL configuration) that cannot be recognized in DADF stream reading mode.
Use case | - Upon user's request - When picking up special paper size original from DADF
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 10 [Inch type] 0: LEGAL-R, 1: FOOLSCAP-R, 2: OFICIO-R, 3: FOLIO-R, 4: Australian FOOLSCAP-R, 5: Ecuador OFICIO-R, 6: Bolivia OFICIO-R, 7: Argentine OFICIO-R, 8: Argentine LEGAL-R, 9: Government LEGAL-R, 10: Mexico OFICIO-R [AB/Inch type] 0: LEGAL-R, 1: FOOLSCAP-R, 2: F4A
Default value | 0
ORG-LTR | Special paper size set in DADF mode: LTR
Lv.2 | Details | To set the size of special paper (LTR configuration) that cannot be recognized in DADF stream reading mode.
Use case | - Upon user's request - When picking up special paper size original from DADF
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 3 0: LETTER 1: EXECUTIVE 2: Argentine LETTER 3: Government LETTER
Default value | 0
ORG-LTRR | Special paper size set in DADF mode: LTRR
Lv.2 | Details | To set the size of special paper (LTRR configuration) that cannot be recognized in DADF stream reading mode.
Use case | - Upon user's request - When picking up special paper size original from DADF
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0 : LETTER-R 1 : OFICIO-R 2 : Ecuador-OFICIO-R
Default value | 0
ORG-LDR | Special paper size set in DADF mode: LDR
Lv.2 | Details | To set the size of special paper (LDR configuration) that cannot be recognized in DADF stream reading mode.
Use case | - Upon user's request - When picking up special paper size original from DADF
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: LEDGER-R (11x17) 1: Argentine LETTER
Default value | 0
ORG-B5 | Special paper size set in DADF mode: B5
Lv.2 | Details | To set the size of special paper (B5) that cannot be recognized in DADF stream reading mode.
Use case | - Upon user's request - When picking up special paper size original from DADF
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: B5, 1: Korean government office paper
Default value | 0
MODELSZ2 | Ppr size dtct global support in bookmode
Lv.2 | Details | To set ON/OFF for global support of document size detection in copyboard reading mode.
Use case | Upon user's request (mixed media original with AB/Inch configuration)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Do not use this at the normal service. - The Document Size Sensor (Photo Sensor) is additionally required to correctly detect the document size when the original consists of mixed media (AB/Inch configuration).
Display/adj/set range | 0 to 1 0: Detected with detection size according to location, 1: Detected with AB/Inch mixed media.
Default value | 0
SVMD-ENT | Setting of entry method to service mode
Lv.2 | Details | To set the way to get in service mode to prevent information leak.
Use case | As needed
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: [Settings/Registration] - Pressing [2] and [8] at the same time - [Settings/Registration] 1: [Settings/Registration] - Pressing [4] and [9] at the same time - [Settings/Registration]
Default value | 0
SC-L-CNT | Set large paper judgment reference at scan

Lv.1

Details

To set the judgment reference of the scan counter as to which to use B4 or LTR to determine large size.
The threshold is determined by the combination with the setting of B4-L-CNT.
SC-L-CNT=0, B4-L-CNT=0: paper exceeding B4 is determined as large size, paper with B4 or smaller is determined as small size.
SC-L-CNT=0, B4-L-CNT=1: paper with B4 or larger is determined as large size, paper smaller than B4 is determined as small size.

Use case | As needed
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: B4 size, 1: LTR size
Default value | 0
Related service mode | COPIER> OPTION> USER> B4-L-CNT
KSIZE-SW | Set of Chinese paper (K-size) support
Lv.2 | Details | To set to detect/display the Chinese paper (K size paper: 8K, 16K).
Use case | When using K size paper
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Go through the following: COPIER > OPTION > FNC-SW > MODEL-SZ; and if MODEL-SZ is "0: AB configuration", this mode is enabled.
Display/adj/set range | 0 to 1 0: Not supported, 1: Supported
Default value | 0
Related service mode | COPIER> OPTION> FNC-SW> MODEL-SZ
Supplement/memo | 8K paper: 270 x 390 mm, 16K paper: 270 x 195 mm
ORG-B4 | Setting of special paper size (B4 type) with DADF
Lv.2 | Details | Setting of special paper size (B4 type) which cannot be recognized when using DADF
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0:JIS B4-R 1:FOLIO-R
Default value | 0
PDF-RDCT | PDF reduction set at forwarding
Lv.2 | Details | To set whether to reduce the image for transmission when converting the image received by IFAX into PDF for e-mail/file transmission.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Following the current setting, 1: Image reduction
Default value | 0
REBOOTSW | Restart setting at E240 error occurrence
Lv.2 | Details | To set whether to reboot in the case of E240 error. In the case of E240 error, the machine is automatically rebooted due to the possibility of continuous operation of the drive system while the spooled print job is cleared. Print job can be obtained if selecting the setting not to reboot.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Do not use this at the normal service. - Be sure to get approval from the user by telling the possibility of continuous operation of the drive system in the case of E240 error.
Display/adj/set range | 0 to 1 0: Rebooted, 1: Not rebooted
Default value | 0
Supplement/memo | E240 error: Communication error between the Main Controller and the DC Controller.
SJB-UNW | Reserve upper limit of secure print job
Lv.2 | Details | To set the upper limit for the number of reserved jobs in secure print job.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: 50 jobs, 1: 90 jobs
Default value | 0
WEBV-SW | ON/OFF of WebDAV function

Lv.2

Details

To set ON/OFF of WebDAV function.
OFF setting can reduce memory use of the machine. In addition, the following WebDAV-related items are hidden in user mode.
- Settings/Registration> Set Destination> Register Destinations> Register New Dest.> File> Protocol> WebDAV
- Settings/Registration> Function Settings> Send> Common Settings> Use Divided Chunk Send for WebDAV TX

Use case | When reducing memory use of the machine
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: ON, 1: OFF
Default value | 0
Related user mode | Settings/Registration> Set Destination> Register Destinations> Register New Dest.> File> Protocol> WebDAV Settings/Registration> Function Settings> Send> Common Settings> Use Divided Chunk Send for WebDAV TX
Supplement/memo | WebDAV function is equipped as standard with the machine.
CARD-RNG | Card number setting (department number)
Lv.2 | Details | To set the number of cards (departments) that can be used with the Card Reader.
Use case | When setting the number of cards (departments)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 1000
Default value | 1000
SJOB-CL | Set of scan job canceling by logout
Lv.1 | Details | To set whether to cancel the scan job in operation by logout of the user.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - The job in scanning operation cannot be canceled. - Cancel by logout is kept in the log.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
Supplement/memo | Scan job: A job after the scanning operation is completed.
USB-RCNT | Auto connect set at USB device disconnct

Lv.2

Details

To set to enable/disable automatic connection when the USB device is disconnected.
With the setting to disable automatic connection, USB device cannot be used if disconnecting and then connecting the USB device. To enable connection again, the power needs to be turned OFF/ON.
With the setting to enable automatic connection, reconnection is made after disconnecting, and then connecting the USB device.

Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | With the setting to enable automatic connection, disconnecting of 1 area makes automatic connection of all USB devices if there is USB hub.
Display/adj/set range | 0 to 1 0: No automatic connection, 1: Automatic connection
Default value | 0
MIBCOUNT | Scope range set of Charge Counter MIB
Lv.2 | Details | To set the range of counter information that can be obtained as MIB (Management Information Base).
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: All charge counters are obtained, 1: Only displayed counter* is obtained, 2: All charge counters are not obtained * : Counter specified by the following: COPIER > OPTION > USER > COUNTER 1 to 6
Default value | 0
Related service mode | COPIER> OPTION> USER> COUNTER1 to 6
CNTR-SW | Init of parts counter replacement timing
Lv.1 | Details | To return the estimated life of parts counter to the initial value.
Use case | Upon user's request
Adj/set/operate method | 1) Enter 0, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: Returned to the initial value
Default value | 0
ILSZ-JAM | ON/OFF of size difference jam detection
Lv.2 | Details | To set ON/OFF of size difference jam detection.
Display/adj/set range | 0 to 1 0: ON, 1: OFF
Default value | 0
W/RAID | Setting of RAID Board installation
Lv.1 | Details | To set installation condition of RAID Board (HDD Mirroring Kit). Select ""1: Installed"" when installing the RAID Board. Select ""0: Not installed"" when removing the RAID Board.
Use case | When installing/removing RAID Board
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Not installed, 1: Installed
Default value | 0
PSWD-SW | Password type set to enter service mode
Lv.1 | Details | To set the type of password that is required to enter when getting into service mode. 2 types are available: one for ""service technician"" and the other for ""system administrator + service technician"". When selecting the type for ""system administrator + service technician"", enter the password for service technician after the password entry by the user's system administrator.
Use case | Upon request from the user who concerns security
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: No password, 1: Service technician, 2: System administrator + service technician
Default value | 0
SM-PSWD | Password setting for service technician
Lv.2 | Details | To set password for service technician that is used when getting into service mode.
Use case | When password is required to get into service mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to select 1 or 2 with PSWD-SW in advance.
Display/adj/set range | 1 to 99999999
Default value | 11111111
Related service mode | COPIER> OPTION> FNC-SW> PSWD-SW
RPT2SIDE | Set of report 1-sided/2-sided output
Lv.1 | Details | To set whether to use 1-sided or 2-sided for report output of service mode.
Use case | When making 2-sided report output to reduce the number of output pages
Display/adj/set range | 0 to 1 0: 1-sided, 1: 2-sided
Default value | 1
Related service mode | COPIER> FUNCTION> MISC-P> P-PRINT
BRWS-FAV | Set of service browser favorite register
Lv.2 | Details | To set whether to allow registration of favorites in the browser for service. When 1 is set, favorites in the browser for service can be edited, and any URLs can be accessed.
Use case | When service engineers edit favorites in the browser for service
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
INVALPDL | Disable of PDL license
Lv.1 | Details | To disable the registered PDL license. When ""1: Disabled"" is set, PDL is disabled even if a PDL license is registered. This is set to the machines installed at convenience stores, which do not allow PDL to be used.
Use case | When prohibiting the use of PDL
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Registered PDL license is enabled, 1: Disabled
Default value | 0
CDS-FIRM | Set to allow firmware update by admin
Lv.1 | Details | To set whether to permit update of the firmware by user (administrator). When ""1: Enabled"" is set, Updater can be activated from the user mode.
Use case | When allowing the administrator to update the firmware
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | Europe: 1, Other than Europe: 0
CDS-MEAP | Set to allow MEAP installation by admin
Lv.1 | Details | To set whether to permit the user (administrator) to install MEAP applications and enable iR options from CDS. When ""1: Enabled"" is set, Updater can be activated from the user mode.
Use case | When allowing the administrator to install MEAP applications and enable iR options from CDS
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled (This setting can be specified for China, Korea and Taiwan models only.)
Default value | 1
Supplement/memo | CDS: Contents Delivery System
CDS-UGW | Set to allow firmware update from UGW
Lv.1 | Details | To set whether to permit update of the firmware from the UGW server. When ""1: Enabled"" is set, Updater accepts the operation from the UGW server in cooperation with CDS.
Use case | When allowing update of the firmware from the UGW server
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
Supplement/memo | CDS: Contents Delivery System
LOCLFIRM | Set to allow firmware update by file
Lv.1 | Details | To set whether to permit the user (administrator) to update the firmware from the remote UI using a local file. This update is executed as a measure for vulnerability in emergency situations.
Use case | When allowing the administrator to update the firmware using a file
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 1
BXNUPLOG | ON/OFF of Nup log at Inbox print
Lv.2 | Details | To set whether to keep Nup log at Inbox print.
Use case | When keeping Nup log at Inbox print
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | At normal service: 0, At customization: 1
SDLMTWRN | Cpcty warn dis ON/OFF at E-mail/I-Fax TX
Lv.1 | Details | To set whether to display the warning message when sending data that exceeds the upper limit value for the transmission data size via E-mail/I-Fax.
Use case | For customization
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
Related user mode | Function Settings> Send> E-Mail/I-Fax Settings> Maximum Data Size for Sending
JLK-PWSC | ON/OFF of PCAM password auth doc scan
Lv.2 | Details | To set whether to scan the PCAM password authentication document with the MEAP application.
Use case | When scanning the PCAM password authentication document
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
FAX-INT | Set FAX RX print interruption oprtn mode
Lv.2 | Details | To set the mode performing interruption operation of FAX reception print automatically.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Normal, 1: Interruption operation mode
Default value | 0
CDS-LVUP | ON/OFF of CDS periodical update function
Lv.1 | Details | To set ON/OFF of periodical update function by CDS. If 1 is set, Updater automatically updates on a periodical basis. Administrator can use the periodical update function from the user mode.
Use case | When allowing the administrator to use the periodical update function
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | Other than Europe: 0, Europe: 1
WTM-DENS | Set density at watermark/PCMA setting
Lv.2 | Details | When the watermark/PCAM is set, the density becomes high by changing the developing /primary charge DC voltage so that the watermark/PCAM is reappeared.
Use case | To increased the density when the watermark/PCAM is selected at the security print mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0
AMSOFFSW | Set AMS(ACQ) mode to OFF
Lv.2 | Details | 1) AMS license of iR-option is installed 2) Login application for AMS is started The device is set to the AMS mode automatically in the above conditions. Use this mode to turn the AMS mode off.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0
UA-OFFSW | ON/OFF of unified auth function
Lv.1 | Details | To set ON/OFF of the Unified Authentication function. Set 0 when not preferring to use the Unified Authentication function because of security concern.
Use case | Upon user's request (not to use the Unified Authentication function)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: ON, 1: OFF
Default value | 0
MIB-NVTA | RFC-compatible character stringMIB write

Lv.1

Details

As default, MIB object which NVT-ASCII can be written exists in order to link with LUI entry value. This violates RFC order, so a problem like garbled 2-byte characters may occur in the SNMP monitoring system, such as the 3rd vendor's MPS.
Whether non-RFC-compatible character strings are written in MIB can be set using this mode.
When 1 is set, only the character strings which are strictly compatible with RFC are written. (Writing operation is executed from the SNMP manager.) LUI is not linked.

Use case | Upon user's request (operation with RFC-compatible system)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch."
Display/adj/set range | 0 to 3 0: Compatible in a conventional manner, 1: RFC-compatible, 2 to 3: Not used
Default value | 0
MIB-EXT | ON/OFF of link with Ex-Cont on network
Lv.1 | Details | To set whether to link with External Controller on network (Hewlett-Packard Co.).
Use case | When linking with External Controller of Hewlett-Packard Co.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: OFF, 1: ON, 2: Not used
Default value | 0
BXSHIFT | Setting of binding at 0mm binding margin

Lv.1

Details

To set whether to judge the job as a job "without binding" when storing a PDL job in Inbox while the binding margin is set to "0".
By setting the binding margin to 0 mm while "0" is set, the job is processed as "without binding". "Booklet" in "Other Functions" on the Inbox screen can be also used.
When "1" is set, it is judged as "with binding" even the binding margin is 0 mm so "Booklet", which has an exclusive relationship with "binding", cannot be used.

Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | When storing a PDL job in Inbox while 1 is set, "Booklet" in "Other Functions" on the Inbox screen cannot be used.
Display/adj/set range | 0 to 1 0: Without binding, 1: With binding
Default value | 0