Operation Check

| Print out this category

Operation Check
NOTE:
To the Multimedia Reader/Writer, Memory Media of the SC Card, Memory Stick, and CF Card can be connected.
With one of the 3 types of Memory Media, perform the oepration check 1 through 3.
When "System Manager Information Settings" is set, be sure to follow the direction of user administrator in order to log in as an administrator.
1.Writing Check
1) Select "1" for the following service mode (Level 2) COPIER > OPTION > DSPLY-SW > UI-MEM
2) To make the setting value effective, turn OFF/ON the main power of the Host Machine.
3) Mount the Memory Media to the Multimedia Card Reader/Writer. (Check that the Mount Mark is indicated in the bottom right.)
4) Make the following selection:[Scan and Store] > [Memory Media] > [Memory Media (A:)]
5) Set originals to DADF (or Copyboard), and press the [Scan] button. Then, press the Start button on the Control Panel.
6) After the completion of original reading, check that the data is stored in the media. After that, press the [Main Menu] button on the Control Panel.
2.Reading Check
7) Make the following selection from Main Menu: [Access Stored Files] > [Memory Media] > [Memory Media(A:)]
8) Select the files stored in step 7) and 8), and then press the [Print] button.
9) Press the [Start Printing] button, and print the file. Then check that the file is printed correctly.
10) Press the [Main Menu] button on the Control Panel.
3.Memory Media Removal
11) Press the [Mount Mark ] in the bottom right.Then, select the memory media to be removed, and press the [Remove] button.
12) ress the [OK] button. Then, check that the Mount Mark is not indicated in the bottom right on the Main Menu screen.