Waste Toner Full Level Detection

| Print out this category

Waste Toner Full Level Detection

Status | Detection timing | Detecting to (location) | Operation
Warning for full level of waste toner (Approx. 99% of the full criterion) | When the Switch is pressed and the total counter value exceeds 50,000 sheets | Waste toner full sensor (S17) | Continuous printing is enabled. (Please prepare a waste toner container)
Full level of waste toner (Full criterion) | When 2,000 sheets are printed since the full level warning. | The number of prints | Host machine is stopped (error display).
When the Switch is pressed and the total counter value fails 50,000 sheets *1 | Waste toner full sensor (S17)

When replacing a waste toner container and the waste toner full sensor detects absence of waste toner after the waste toner full sensor detected presence of a waste toner container, the counter of the waste toner container is cleared. When replacing a waste toner container before the alert, be sure to clear the following in service mode: COUNTER > DRBL-1 > WST-TNR
*1: Special full level detection
When attaching a waste toner container that has been used by the other machine, or the counter information is lost for some reason, it is necessary to notify full level before an alert is given. (The counter shows less than 50,000 although the sensor detects full level of waste toner) In such a case, it is determined as full level without an alert and the machine cannot continue printing.
Explain the user that there will be no alert when any of the above is executed.