﻿Removing the Manual Feed Pickup Roller

| Print out this category

Removing the Manual Feed Pickup Roller
CAUTION:
Do not touch the roller surface during work.
1) Remove the manual feed pickup roller cover.
1 screw
2) Release the claws, and then slide the bushing (front).
3) Remove the manual feed pickup roller.
1 claw
NOTE:
Reassemble the manual feed pickup roller as shown.
1. Fit the hole of the manual feed pickup roller to the projection of the bushing (rear) and attach it.
2. Press down the separation pad.
3. Attach the bushing (front) to the manual feed pickup roller.
NOTE:
When replacing the consumable parts, be sure to clear the parts counter.
(COPIER > COUNTER > DRBL-1 > M-FD-RL)