Main Body_DC controller (DC-CON>P001 to P016)

| Print out this category

I/O
Main Body_DC controller (DC-CON>P001 to P016)
Main Body
Cassette Feeding Unit-AF1
Buffer Pass Unit-H1
Paper Deck Unit-B2

Address | bit | Name | Symbol | Remarks
P001 | 15 | Cassette 1 Paper Width Detection Switch 4 | S35 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
14 | Cassette 1 Paper Width Detection Switch 3
13 | Cassette 1 Paper Width Detection Switch 2
12 | Cassette 1 Paper Width Detection Switch 1
11 | Cassette 1 Paper Length Detection Switch 4 | S30 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
10 | Cassette 1 Paper Length Detection Switch 3
9 | Cassette 1 Paper Length Detection Switch 2
8 | Cassette 1 Paper Length Detection Switch 1
7 | Pre-Registration Sensor | S5 | 0:Paper presence
6 | Cassette 1 Pickup Sensor | S1 | 0:Paper presence
5 | Cassette 1 Paper Sensor | S2 | Detect paper level by combination of 3 sensors 0: ON 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual
4 | Cassette 1 Paper Level Sensor B | S3
3 | Cassette 1 Paper Level Sensor A | S4
2 | Loop Sensor | S6 | 1:Paper presence
1 | Duplex Feed Sensor | S7 | 1:Paper presence
0 | Not used |  |
P002 | 15 | Manual Feeder Paper Sensor | S9 | 0:Paper presence
14 | Exhaust Fan (Front) Lock Detect Signal | FM4 | 0:Lock
13 | Exhaust Fan (Rear) Lock Detect Signal | FM3 | 0:Lock
12 | Reversal Sensor | S24 | 1:Paper presence
11 | No.2 Delivery Full Sensor | S23 | 0:Non-full
10 | No.2 Delivery Sensor | S22 | 1:Paper presence
9 | No.1 Delivery Full Sensor | S20 | 0:Non-full
8 | No.1 Delivery Sensor | S21 | 1:Paper presence
7 | Wste Toner Sensor | S17 | 1:Full
6 | Developing Assembly Toner Sensor | S25 | 1:Toner presence
5 | Developing Assembly Toner Sensor Connect Detect Signal | S25 | 0:Not connect
4 | Sub Hopper Toner Sensor | S26 | 1:Toner presence
3 | Sub Hopper Toner Sensor Connect Detect Signal | S26 | 0:Not connect
2 | Hopper Motor Error Detct Signal | M16 | 1:Error
1 | Bottle Motor Error Detct Signal | M17 | 1:Error
0 | Paper Cooling Fan Lock Detect Signal | FM7 | 0:Lock
P003 | 15 | For R&D use |  |
14 | Buffer Pass Motor Drive Permission Signal | M101 | 1:Drive permission
13 | For R&D use |  |
12 | For R&D use |  |
11 | For R&D use |  |
10 | For R&D use |  |
9 | Bottle Motor Error Latch Release Signal | M17 | 1:Latch release
8 | Cassette 1 Pickup Motor Drive Permission Signal | M13 | 0:Drive permission
7 | Duplex Feed Motor Drive Permission Signal | M9 | 0:Drive permission
6 | No.1 Delivery Motor Drive Permission Signal | M10 | 0:Drive permission
5 | For R&D use |  |
4 | For R&D use |  |
3 | Hopper Motor Drive Signal | M16 | 1:Drive
2 | Bottle Motor Drive Signal | M17 | 1:Drive
1 | Paper Cooling Fan Half Speed Drive Signal | FM7 | 1:Half speed drive
0 | Paper Cooling Fan Full Speed Drive Signal | FM7 | 1:Full speed drive
P004 | 15 | For R&D use |  |
14 | For R&D use |  |
13 | Reversal Motor Drive Permission Signal | M20 | 1:Drive permission
12 | Exhaust Fan Half Speed Drive Signal | FM3/4 | 1:Half speed drive
11 | Exhaust Fan Full Speed Drive Signal | FM3/4 | 1:Full speed drive
10 | Manual Feed Pickup Solenoid Drive Signal | SL2 | 1:Drive
9 | For R&D use |  |
8 | For R&D use |  |
7 | For R&D use |  |
6 | For R&D use |  |
5 | Manual Feed Pickup Clutch Drive Signal | CL12 | 1:Drive
4 | Developing Cylinder Clutch Drive Signal | CL1 | 1:Drive
3 | Registration Clutch Drive Signal | CL3 | 1:Drive
2 | Cassette 1 Pickup Solenoid Drive Signal | SL1 | 1:Drive
1 | Fixing Motor Break Signal | M2 | 1:Brake
0 | Main Motor Break Signal | M1 | 1:Brake
P005 | 15 | For R&D use |  |
14 | For R&D use |  |
13 | For R&D use |  |
12 | For R&D use |  |
11 | For R&D use |  |
10 | Laser Scanner Unit Connection Detection | - | 0:Connect
9 | For R&D use |  |
8 | Paper Edge Cooling Fan (Front) Lock Detect Signal | FM2 | 0:Lock
7 | Paper Edge Cooling Fan (Rear) Lock Detect Signal | FM1 | 0:Lock
6 | Paper Edge Shutter HP Sensor | S10 | 0:HP
5 | Fixing Outlet Sensor | S19 | 0:Paper absence
4 | Polygon Motor Speed Lock Detect Signal | M11 | 0:Lock
3 | Main Body Cooling Fan Lock Detect Signal | FM6 | 0:Lock
2 | Fixing Motor Speed Lock Detect Signal | M2 | 1:Lock
1 | Main Motor Speed Lock Detect Signal | M1 | 1:Lock
0 | Cassette Cover Sensor Open/Close Detect Signal | S39 | 0:Open
P006 | 15 | Buffer Pass Unit Connection Detection | - | 0:Connect
14 | Buffer Pass Paper Out Sensor | SR3 | 1:Paper absence
13 | Buffer Pass Paper In Sensor | SR2 | 1:Paper absence
12 | Buffer Pass Open Sensor | SR1 | 0:Open
11 | Cassette 2 Pickup Sensor | S33 | 1:Paper presence
10 | Cassette 2 Paper Sensor | S31 | Detect paper level by combination of 3 sensors 0: ON 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual
9 | Cassette 2 Paper Level Sensor B | S34
8 | Cassette 2 Paper Level Sensor A | S32
7 | Cassette 2 Paper Width Detection Switch 4 | S28 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
6 | Cassette 2 Paper Width Detection Switch 3
5 | Cassette 2 Paper Width Detection Switch 2
4 | Cassette 2 Paper Width Detection Switch 1
3 | Cassette 2 Paper Length Detection Switch 4 | S29 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
2 | Cassette 2 Paper Length Detection Switch 3
1 | Cassette 2 Paper Length Detection Switch 2
0 | Cassette 2 Paper Length Detection Switch 1
P007 | 15 | Cassette 3 Paper Width Detection Switch 4 | SW102 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
14 | Cassette 3 Paper Width Detection Switch 3
13 | Cassette 3 Paper Width Detection Switch 2
12 | Cassette 3 Paper Width Detection Switch 1
11 | Cassette 3 Paper Length Detection Switch 4 | SW101 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
10 | Cassette 3 Paper Length Detection Switch 3
9 | Cassette 3 Paper Length Detection Switch 2
8 | Cassette 3 Paper Length Detection Switch 1
7 | Cassette 4 Paper Width Detection Switch 4 | SW104 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
6 | Cassette 4 Paper Width Detection Switch 3
5 | Cassette 4 Paper Width Detection Switch 2
4 | Cassette 4 Paper Width Detection Switch 1
3 | Cassette 4 Paper Length Detection Switch 4 | SW103 | Detect paper size by combination of 4 switches 0: ON (Condition that the switch is pressed) 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual.
2 | Cassette 4 Paper Length Detection Switch 3
1 | Cassette 4 Paper Length Detection Switch 2
0 | Cassette 4 Paper Length Detection Switch 1
P008 | 15 | Cassette 2 Pickup Solenoid Drive Signal | SL11 | 1:Drive
14 | Paper Edge Cooling Fan Half Speed Drive Signal | FM1/2 | 1:Drive
13 | Cassette 2 Pickup Motor Drive Permission Signal | M3 | 1:Drive permission
12 | For R&D use |  |
11 | For R&D use |  |
10 | Paper Edge Cooling Fan Full Speed Drive Signal | FM1/2 | 1:Drive
9 | For R&D use |  |
8 | For R&D use |  |
7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
P009 | 15 | Cassette 3 Paper Sensor | PS102 | Detect paper level by combination of 3 sensors 0: ON 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual
14 | Cassette 3 Paper Level Sensor A | PS104
13 | Cassette 3 Paper Level Sensor B | PS105
12 | Cassette 3 Retry Sensor | PS108 | 1:Paper presence
11 | Cassette 4 Paper Sensor | PS103 | Detect paper level by combination of 3 sensors 0: ON 1: OFF As for the combination, refer to the Pickup/Feed System in Service Manual
10 | Cassette 4 Paper Level Sensor A | PS106
9 | Cassette 4 Paper Level Sensor B | PS107
8 | Cassette 4 Retry Sensor | PS109 | 1:Paper presence
7 | Pedestal Right Cover Sensor Open/Close Detect Signal | PS101 | 0:Open
6 | Not used |  |
5 | Paper Deck Connection Detection | - | 1:Separation From the Host Machine
4 | Deck Paper Level Sensor | PS7D | 1:Paper absence
3 | Deck Paper Replenishing Position Sensor | PS8D | 1:Paper absence
2 | Deck Pickup Sensor | PS6D | 0:Paper presence
1 | Deck Paper-out Sensor | PS2D | 1:Paper absence
0 | Deck Open Switch | SW100D | 1:Push
P010 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | Deck Open Solenoid Drive Signal | SL2D | 1:Drive
3 | For R&D use |  |
2 | Polygon Motor Drive Signal | M11 | 1:Drive
1 | Fixing Motor Drive Signal | M2 | 1:Drive
0 | Main Motor Drive Signal | M1 | 1:Drive
P011 | 7 | Enviorment Heater Drive Signal |  | 1:Heater OFF
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Relay Drive Signal | - | 0:Relay ON
P012 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | Fixing Main Thermistor Connect Detect Siganal | TH1 | 0:Connect
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Enviorment Heater Connect Detect Siganal | S16 | 0:Connect
P013 | 7 | Fixing Sub Thermistor 2 Error Detect Signal | TH3 | 1:Normal
6 | For R&D use |  |
5 | Fixing Sub Thermistor 1 Error Detect Signal | TH2 | 1:Normal
4 | Fixing Main Thermistor Error Detect Signal | TH1 | 1:Normal
3 | Front Cover Open/Closed Sensor | S18 | 1:Close
2 | Toner Cover Open/Closed Sensor | S46 | 1:Close
1 | For R&D use |  |
0 | Main Switch/Front Door Switch | SW1/SW2 | 1:Open
P014 | 7 | For R&D use |  |
6 | Deck Lifter Motor Drive Signal | M2D | 0:Drive
5 | Deck Pickup Clutch Drive Signal | CL2D | 1:Drive
4 | Deck Pickup Roller Release Solenoid Drive Signal | SL1D | 1:Drive
3 | For R&D use |  |
2 | Hopper Motor Error Latch Signal | M16 | 1:Latch release
1 | Main Body Cooling Fan Half Speed Drive Signal | FM6 | 1:Drive
0 | Main Body Cooling Fan Full Speed Drive Signal | FM6 | 1:Drive
P015 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Cassette 3 Pickup Motor Drive Permission Signal | M101 | 0:Drive permission
2 | Cassette 4 Pickup Motor Drive Permission Signal | M102 | 0:Drive permission
1 | Cassette 4 Pickup Solenoid Drive Signal | SL102 | 1:Drive
0 | Cassette 3 Pickup Solenoid | SL101 | 1:Drive
P016 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | Deck Lifter Lower Limit Sensing Switch | SW2D | 0:Lower limit
4 | Deck Lifter Upper Limit Sensor | PS3D | 0:Upper limit
3 | Deck Lifter Position Sensor | PS4D | 0:Lifter position
2 | Deck Feed Sensor | PS1D | 0:Paper presence
1 | Not used |  |
0 | Deck Open Sensor | PS9D | 1:Open